For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the seat cushion inner trim panel. Refer to Seat Cushion Inner Trim Panel Replacement .
3. Remove the seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement .

1 | Bolt, Seat Belt Buckle Tighten 45 N·m (33 lb ft)
2 | Buckle Assembly, Seat Belt