For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Refrigerant Pressure Sensor | 5 N·m | 44 lb in
Blower Motor Mounting Screws | 1.8 N·m | 16 lb in
Blower Motor Nuts | 2.4 N·m | 21 lb in
Blower Resister Mounting Screws | 1.8 N·m | 16 lb in
Center Air Distribution Duct Retaining Screws | 2.5 N·m | 22 lb in
Charge Air Cooler Inlet Hose Clamp - To Turbo | 9 N·m | 80 lb in
Charge Air Cooler Inlet Hose Clamp - To Cooler | 6 N·m | 53 lb in
Charge Air Cooler Outlet Hose Clamp - To Cooler | 6 N·m | 53 lb in
Charge Air Cooler Outlet Hose Clamp - To Throttle Body | 5 N·m | 44 lb in
Charge Air Cooler Pump Mounting Clamp Bolt | 10 N·m | 89 lb in
Compressor Clutch Drive Plate Bolt | 12 N·m | 106 lb in
Compressor Drain Plug | 16 N·m | 12 lb ft
Compressor Hose to Compressor Bolt | 20 N·m | 15 lb ft
Compressor Hose to Condenser Bolt | 20 N·m | 15 lb ft
Compressor Hose to Evaporator Hose Nut | 20 N·m | 15 lb ft
Compressor Mounting Bolts | 25 N·m | 18 lb ft
Compressor Pressure Relief Valve | 7 N·m | 62 lb in
Condenser Mounting Bolts | 10 N·m | 88 lb in
Defroster Duct Retaining Screws | 2.5 N·m | 22 lb in
Evaporator Inlet Line Clamp Nut | 10 N·m | 88 lb in
Evaporator Inlet Line to Condenser Bolt | 20 N·m | 15 lb ft
Evaporator Outlet Line to TXV Nut | 20 N·m | 15 lb ft
Heater Core Cover Screws | 1.8 N·m | 16 lb in
HVAC Module Actuator Screws | 1.8 N·m | 16 lb in
HVAC Module Case Screws | 1.8 N·m | 16 lb in
HVAC Module to Cross Vehicle Beam Mounting Bolts | 10 N·m | 88 lb in
HVAC Module to Dash Panel Nuts | 10 N·m | 88 lb in
Instrument Panel (I/P) Carrier Bolts | 25 N·m | 18 lb ft
Outer Air Outlet Duct Retaining Screws | 2.5 N·m | 22 lb in
Service Port Valve Core | 2.5 N·m | 22 lb in
Side Window Duct Retaining Screws | 2.5 N·m | 22 lb in
TXV to Evaporator Core Mounting Bolts | 7 N·m | 62 lb in