For 1990-2009 cars

### Removal Procedure

1. Loosen the outlet duct clamp at the air cleaner assembly.
2. Remove the push pin (1).
3. Remove the air cleaner mounting nuts (2).
4. Remove the air cleaner.

### Installation Procedure

Important: Verify full engagement of the inlet onto the resonator neck.

1. Position the air cleaner assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air cleaner assembly attachment nut (2).

Tighten
Tighten the nut to 10 N·m (89 lb in).

3. Install the push pin (1).
4. Connect the air cleaner resonator to the air cleaner assembly.

Tighten
Tighten the air cleaner intake duct clamp to 5 N·m (44 lb in).