For 1990-2009 cars

#### Tools Required

• | 87 91 204 Output Shaft Bearing Race Sleeve

• | 87 91 220 Drift, Main Shift Rod Bushing

• | 87 92 236 Support

1. Press out the input shaft bearing race using the 87 91 204 . Use the 87 92 236 as a base for pressing operation.
2. Tap out the axle seal and discard.

Important: When driving to the differential bearing race, tap equally on the opposite sides of the race to avoid damaging the race bore and seal surface.

3. Tap out the differential bearing race using a punch and hammer.