For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Bolt | 10 N·m | 89 lb in
Air Cleaner Housing Rear Bolt | 10 N·m | 89 lb in
Air Cleaner Intake Duct Bolt | 10 N·m | 89 lb in
Air Cleaner Outlet Duct Clamp | 4 N·m | 35 lb in
Camshaft Position (CMP) Actuator Solenoid Valve Bolt | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 10 N·m | 89 lb in
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Evaporative Emission (EVAP) Canister Bolt | 3.5 N·m | 35 lb in
Evaporative Emission (EVAP) Canister Purge Valve Bracket Bolt | 25 N·m | 18 lb ft
Frame (Rear) Bolt - First Pass | 100 N·m | 74 lb ft
Frame (Rear) Bolt - Final Pass | 90 Degrees
Fuel Fill Pipe Hose Clamp | 4 N·m | 35 lb in
Fuel Rail Bolt | 10 N·m | 89 lb in
Fuel Tank Fill Pipe Bracket Bolt | 9 N·m | 80 lb in
Fuel Tank Fill Pipe to Fuel Tank Fill Pipe Housing Screw | 1.5 N·m | 13 lb in
Fuel Tank Strap Bolt | 20 N·m | 15 lb ft
Heated Oxygen Sensor (HO2S) | 42 N·m | 31 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor (KS) | 25 N·m | 18 lb ft
Mass Air Flow (MAF)/Intake Air Temperature (IAT) Sensor Screw | 0.6 N·m | 5 lb in
Secondary Air Injection Check Valve Bolt | 10 N·m | 89 lb in
Secondary Air Injection Check Valve Nut | 25 N·m | 18 lb ft
Secondary Air Injection Pipe Bolt | 10 N·m | 89 lb in
Secondary Air Injection Pump Bolt | 30 N·m | 22 lb ft
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in