For 1990-2009 cars

### Removal Procedure

1. Loosen the air cleaner assembly air duct at the outlet duct clamp (1).
2. Loosen the outlet duct clamp (2) at the throttle body.
3. Remove the air outlet duct.

### Installation Procedure

1. Install the air outlet duct.
2. Install the air outlet duct clamps (1 and 2).

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the air outlet duct clamps (1 and 2).

Tighten
Tighten the clamps to 5 N·m (44 lb in).