For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the seat cushion inner trim cover. Refer to Seat Cushion Inner Trim Panel Replacement .
3. Remove the seat cushion outer trim cover. Refer to Front Seat Cushion Outer Trim Panel Replacement .
4. Remove the front seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement .
5. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Passenger Presence System Programming and Setup .

1 | Screw, Seat Cushion Assembly (Qty: 4) Tighten 25 N·m (18 lb ft)
2 | Frame Assembly, Seat Cushion Tip

• | Remove the lumbar adjuster screws.

• | Disconnect the cushion heater electrical connector.