For 1990-2009 cars

## Rear Bumper Fascia Bracket Replacement Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.

1 | Rear Bumper Fascia Center Bracket Nut (Qty: 5) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Bumper Fascia Center Bracket
3 | Rear Bumper Fascia Side Bracket Bolt (Qty: 4) Tighten 2.5 N·m (22 lb ft)
4 | Rear Bumper Fascia Side Bracket
5 | Rear Bumper Fascia Upper Bracket Bolt (Qty: 4) Tighten 2.5 N·m (22 lb in)
6 | Rear Bumper Fascia Upper Bracket

## Rear Bumper Fascia Bracket Replacement Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.

1 | Rear Bumper Fascia Side Bracket Bolt (Qty: 4) Caution: Refer to Fastener Caution in the Preface section. Tighten 2.5 N·m (22 lb in)
2 | Rear Bumper Fascia Side Bracket
3 | Rear Bumper Fascia Center Bracket Bolt (Qty: 4) Tip Remove the wiring harness retainers from the studs before removing nuts. Tighten 10 N·m (89 lb in)
4 | Rear Bumper Fascia Center Bracket