For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Rear Side Door Hinge Upper Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tip

1. Support the door before removing the door hinge bolts.
2. Disconnect the door electrical connector.

Tighten
35 N·m (26 lb ft)

2 | Rear Side Door Check Link Bolt Tighten 20 N·m (15 lb ft)
3 | Rear Side Door Hinge Lower Bolt (Qty: 2) Tighten 35 N·m (26 lb ft)
4 | Rear Side Door Assembly Tip When replacing the door it is necessary to transfer all of the internal components.