For 1990-2009 cars

## Door Striker Replacement Coupe

Callout | Component Name
--- | ---
1 | Front Side Door Lock Striker Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Front Side Door Lock Striker Tip Adjust striker as needed. Refer to Door Lock Striker Adjustment .

## Door Striker Replacement Sedan

Callout | Component Name
--- | ---

#### Front Side Door Lock Striker Replacement

1 | Front Side Door Lock Striker Screw (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 25 N·m (18 lb ft)
2 | Front Side Door Lock Striker Tip Adjust striker as needed. Refer to Door Lock Striker Adjustment .

#### Rear Side Door Lock Striker Replacement

3 | Rear Side Door Lock Striker Screw (Qty: 2) Tighten 25 N·m (18 lb ft)
4 | Rear Side Door Lock Striker Tip Adjust striker as needed. Refer to Door Lock Striker Adjustment .