For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement.
3. Move the window to the full up position and secure in place with tape.

1 | Side Door Window Regulator Motor Bolt (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Window Regulator Motor Tip Disconnect the electrical connector.