For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement .

1 | Rear Side Door Lock Assembly Refer to Rear Door Lock Replacement .
2 | Rear Side Door Locking Rod Bellcrank Assembly Tip Disconnect the locking rods from the bellcrank.
3 | Rear Side Door Locking Rod
4 | Rear Side Door Locking Rod
5 | Rear Side Door Locking Rod Cap