For 1990-2009 cars

### Removal Procedure

1. Remove the drive belt. Refer to Drive Belt Replacement .
2. Remove the evaporative emission (EVAP) tube and EVAP valve.
3. Remove the throttle body and gasket. Refer to Throttle Body Assembly Replacement .
4. Remove the supercharger inlet pressure (SCIP) sensor .
5. Disconnect the vacuum brake booster hose.
6. Remove the intercooler fill neck bracket bolts.
7. Remove the vacuum line from the supercharger.
8. Remove the supercharger . Remove the gasket if damaged.

### Installation Procedure

1. Install the supercharger gasket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the supercharger and bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the intercooler fill neck bracket bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Connect the vacuum brake booster hose.
5. Install the SCIP sensor and bolt.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

6. Install the throttle body. Refer to Throttle Body Assembly Replacement .