For 1990-2009 cars

### Removal Procedure

Important: Place the shift control in NEUTRAL before attempting to remove the shift knob screw.

1. Pull the shift knob bezel (1) down to expose the shift knob retaining screw.
2. Remove the shift knob retaining screw (1).
3. Remove the shift knob (1) and bezel (2) from the shift control lever.

### Installation Procedure

Important: Place the shift control in NEUTRAL before attempting to install the shift knob screw.

1. Install the bezel (2) and shift knob (1) to the shift control lever.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the shift knob retaining screw (1).

Tighten
Tighten the screw to 2 N·m (18 lb in).

3. Secure the shift knob bezel (1) to the shift knob.