For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the front seat cushion cover and pad. Refer to Front Seat Cushion Cover and Pad Replacement.
3. Remove the front seat back cover and pad. Refer to Front Seat Back Cushion Cover and Cushion Pad Replacement.

1 | Passenger Seat Adjuster Cable

#### Procedure

1. Disconnect the upper portion of the adjuster cable at the outer recliner.
2. Disconnect the lower portion of the adjuster cable from the bottom side of the seat as shown.