For 1990-2009 cars

## Cooling Fan Always On 2.2L

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Circuit/System Description

The engine control module (ECM) grounds the low speed relay, which is relay 1, and the high speed relay, which is relay 2, control circuits through an internal solid state device called a driver. The primary function of the driver is to supply the ground for the component being controlled. Each driver has a fault line that is monitored by the ECM. When the ECM is commanding a component ON, the voltage potential of the control circuit should be low, near 0 volts. When the ECM is commanding the control circuit to a component OFF, the voltage potential of the circuit should be high, near battery voltage. If the ECM detects that the actual state of the control circuit does not match the expected state, a DTC will set.

### Reference Information

#### Schematic Reference

Engine Cooling Schematics

#### Connector End View Reference

• | Master Electrical Component List

• | Component Connector End Views

#### Description and Operation

Cooling Fan Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

• | Electrical Center Identification Views

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References for scan tool information

### Circuit/System Verification

1. If DTCs P0480 or P0481 are set, then perform those diagnostics first.
2. Ignition ON, verify with a scan tool that the ECM is not commanding fan activation.
3. Ignition ON, observe that the fan is not activated.

### Circuit/System Testing

Note: You must perform the Circuit/System Verification before proceeding with Circuit/System Testing.

1. Ignition OFF, disconnect the relays.
2. Ignition ON, observe that the fan is not activated.

⇒ | If the fan is not activated, replace the faulty relay.

⇒ | If the fan is activated, test the fan voltage supply circuits for a short to voltage.

### Repair Instructions

• | Cooling Fan and Shroud Replacement

• | Cooling Fan and Shroud Replacement

• | Control Module References

### Repair Verification

1. Ignition ON, verify with a scan tool that the ECM is not commanding fan activation.
2. Ignition ON, observe that the fan is not activated.

## Cooling Fan Always On 2.0

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Circuit/System Description

The engine control module (ECM) commands the fans ON in either high speed or low speed, depending on cooling requirements. In low speed, both fans are turned ON at a reduced speed. High speed has both fans turned ON at full speed.

In low speed operation, the ECM applies ground to the coil side of the fan low relay. This energizes the coil and applies voltage directly to the left cooling fan through the switch side of the fan low relay, which is fed by the fan 1 fuse. The right fan is connected in series to the left fan through the de-energized fan control relay so that both operate at low speed.

In high speed operation, the ECM applies a ground to the coil side of the fan low relay, the fan control relay , and the fan high relay. On the fan high relay, the energized coil closes the switch side of the relay and applies voltage directly to the right cooling fan through the switch side of the relay, which is fed by the fan 2 fuse. At the same time, the ECM energizes fan control relay pulling the switch side over, providing a direct path to ground for the left cooling fan, which has voltage applied through the energized fan low relay. In high speed mode, the fans are operated as a parallel circuit with full voltage applied to each.

### Reference Information

#### Schematic Reference

Engine Cooling Schematics

#### Connector End View Reference

Component Connector End Views

#### Description and Operation

Cooling Fan Description and Operation

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

### Circuit/System Verification

1. If DTCs P0480, P0481, P0691, P0692, P0693, or P0694 are set, perform those diagnostics first.
2. Ignition ON, verify with a scan tool that the control module is not commanding fan activation.
3. Ignition ON, observe that the fans are not activated.

### Circuit/System Testing

1. Ignition OFF, disconnect the fan high relay.
2. Ignition ON, observe that both fans are now OFF.

⇒ | If both fans are OFF, replace the fan high relay. If either fan is still activated, remove the fan low relay. If both fans are now OFF replace the fan low relay. If either fan is still activated, test for a short to voltage in the fan voltage supply circuit.

### Repair Verification

1. Ignition ON, verify with a scan tool that the control module is not commanding fan activation.
2. Ignition ON, observe that the fans are not activated.