For 1990-2009 cars

### Removal Procedure

1. Remove the steering column filler panel. Steering Column Opening Filler Replacement.
2. Disconnect the instrument panel (I/P) wiring harness electrical connector from the accelerator pedal position (APP) sensor.
3. Remove the accelerator pedal bolts.
4. Remove the accelerator pedal with sensor.

### Installation Procedure

1. Position the accelerator pedal with sensor.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the accelerator pedal bolts and tighten to 10 N·m (89 lb in).
3. Connect the I/P wiring harness electrical connector to the APP sensor.
4. Install the steering column filler panel. Refer to Steering Column Opening Filler Replacement.