For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the side door window outer sealing strip. Refer to Front Side Door Window Belt Outer Sealing Strip Replacement .

1 | Front Side Door Window Tip

• | Move the window about half way down and loosen the retainer clips that secure the window regulator to the window assembly.

• | Tilt the window inward and remove through the inside of the side door window opening.