For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Rear Side Door Trim Panel Replacement.
2. Remove the water deflector. Refer to Rear Side Door Water Deflector Replacement.

1 | Rear Side Door Window Inner Sealing Strip
2 | Rear Side Door Stationary Window Screw Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
3 | Rear Side Door Window Weatherstrip Assembly Tip Disengage the window and weatherstrip from the door and stationary window.
4 | Rear Side Door Window Bolt (Qty: 2) Tighten 10 N·m (89 lb in)
5 | Rear Side Door Window Tip Tilt the window inward and remove through the inside of the side door window opening.