For 1990-2009 cars

Table 1: | Indicators
Table 2: | Driver Information Center

#### Indicators

Symbol | Reference
--- | ---
| ABS: Refer to ABS Description and Operation
| Air Bag: Refer to SIR System Description and Operation
BRAKE | Brake: Refer to Brake Warning System Description and Operation
| Charge: Refer to Charging System Description and Operation
| Engine Coolant Temperature: Refer to Cooling System Description and Operation
| Engine Oil Pressure: The instrument panel cluster (IPC) illuminates the engine oil pressure (EOP) indicator when the engine oil pressure is below minimum requirements.
| Front Fog Lamps: Refer to Exterior Lighting Systems Description and Operation
| High Beam: Refer to Exterior Lighting Systems Description and Operation
| MIL: Refer to Powertrain Control Module Description for the 2.0L engine, Engine Control Module Description for the 2.2L engine, or Engine Control Module Description for the 2.4L engine
| Seatbelt: Refer to Seat Belt System Description and Operation
| Security: Refer to Theft Systems Description and Operation
| Traction Disabled: Refer to ABS Description and Operation
| Turn Signals: Refer to Exterior Lighting Systems Description and Operation
| Upshift Indicator: The Upshift indicator notifies the driver when to shift the transmission into the next highest gear.

#### Driver Information Center

Message | Reference
--- | ---
AUTO LIGHTS OFF | Refer to Exterior Lighting Systems Description and Operation
AUTO LIGHTS ON | Refer to Exterior Lighting Systems Description and Operation
BATTERY SAVER ACTIVE | Refer to Charging System Description and Operation
BRAKE FLUID | Refer to Brake Warning System Description and Operation
CHARGING SYSTEM ACTIVE | Refer to Charging System Description and Operation
CHANGE OIL SOON | The driver information center (DIC) displays the CHANGE ENGINE OIL message when the engine oil life is 0 percent. .
CHECK GAS CAP | Refer to Evaporative Emission Control System Description for the 2.0L engine, Evaporative Emission Control System Description for the 2.2L engine, or Evaporative Emission Control System Description for the 2.4L engine.
CRUISE CONTROL ACTIVE | Refer to Cruise Control Description and Operation
DOOR AJAR | Refer to Power Door Locks Description and Operation
ENG PWR REDUCED | Refer to Cooling System Description and Operation
ICE POSSIBLE | The driver information center (DIC) displays the ICE POSSIBLE message when the outside air temperature drops below 2°C (36°F). When the temperature rises above 5.5°C (42°F), the ICE POSSIBLE message turns OFF.
KEY FOB BATT LOW | Refer to Keyless Entry System Description and Operation
LOW COOLANT | Refer to Cooling System Description and Operation
LOW FUEL | The driver information center (DIC) displays the low fuel indicator when the fuel level is less than 14 percent.
LOW OIL LEVEL | The driver information center (DIC) displays the LOW OIL LEVEL message when the engine oil level is below minimum requirements.
LOW WASHER FLUID | Refer to Wiper/Washer System Description and Operation
LOW TRACTION | Refer to ABS Description and Operation
POWER STEERING | Refer to Power Steering System Description and Operation
PARKING BRAKE | Refer to Park Brake System Description and Operation
SERVICE AIR BAG | Refer to SIR System Description and Operation
SERVICE VEHICLE SOON | The driver information center (DIC) displays the SERVICE VEHICLE SOON message when certain malfunctions that are not emissions related.
STARTING DISABLED | Refer to Starting System Description and Operation
TRUNK AJAR | Refer to Luggage Compartment Description and Operation