For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Raise the hood.
2. Remove the hood insulator push-in retainers (1) from the hood using the J 38778 .
3. Slide the hood insulator rearward. Remove the hood insulator (2).

### Installation Procedure

1. Position the hood insulator (2) under the tabs that are located at the front and center of the hood.
2. Install the hood insulator push-in retainers (1) until fully seated.
3. Close the hood.