For 1990-2009 cars

Important: Review the system operation in order to familiarize yourself with the system functions. Refer to Wiper/Washer System Description and Operation.

### Visual/Physical Inspection

• | Inspect the washer fluid reservoir for the proper fluid level and condition.

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

• | Inspect for aftermarket devices which could affect the operation of the Windshield Wiper/Washer System.

### Intermittent

• | If the wipers operate at low speed for approximately 3 seconds and then stop, the wiper motor park switch, or its signal circuit, may be malfunctioning.

• | Faulty electrical connections or wiring may be the cause of intermittent conditions. Refer to Testing for Intermittent Conditions and Poor Connections.

### Symptom List

Refer to Windshield Wiper System Malfunction in order to diagnose the symptom.