For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the center instrument trim panel. Refer to Instrument Panel Center Trim Panel Replacement .
2. Remove the HVAC controls.

1 | Radio Screw (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 2 N·m (18 lb in)
2 | Radio

#### Procedure

1. Disconnect the electrical and antenna connectors.
2. Reprogram the radio. Refer to Control Module References .

Tip
The HVAC control connector-1 and the radio connector-2 can be interchanged. Mark or place tape on the connector to avoid accidental interchange.