For 1990-2009 cars

# Diagnostic information for Intermittent Restraints, Air Bag (SIR) Indicator/Lamp On with DTC(s) B0012, B0013, B0014, B0016, B0019, B0020, B0022, B0023, B0026, B0033, B0040, B0042 or B0044 Set

Subject: | Diagnostic Information for Intermittent Restraints, Air Bag (SIR) Indicator/Lamp On with DTC(s) B0012, B0013, B0014, B0016, B0019, B0020, B0022, B0023, B0026, B0033, B0040, B0042 or B0044 Set

Models: | 2005-2007 Buick Rainier

| 2006-2009 Buick Allure, LaCrosse, Lucerne

| 2008-2009 Buick Enclave

| 2006-2009 Cadillac DTS

| 2007-2009 Cadillac Escalade Models

| 2008-2009 Cadillac CTS, SRX, STS, XLR

| 2005-2006 Chevrolet SSR

| 2005-2009 Chevrolet Cobalt, Trailblazer, Trailblazer EXT

| 2006-2007 Chevrolet Monte Carlo

| 2006-2009 Chevrolet Corvette, HHR, Impala, Malibu Models (includes Malibu Classic)

| 2007-2009 Chevrolet Avalanche, Equinox, Silverado, Suburban, Tahoe

| 2008-2009 Chevrolet Express

| 2005-2009 GMC Envoy Models

| 2007-2009 GMC Acadia, Sierra, Yukon, Yukon Denali, Yukon XL, Yukon Denali XL

| 2008-2009 GMC Savana

| 2005-2006 Pontiac Pursuit

| 2006-2009 Pontiac Solstice

| 2007-2009 Pontiac G5, Torrent

| 2008-2009 Pontiac G8

| 2005-2009 Saab 9-7X

| 2007-2009 Saturn AURA, OUTLOOK, SKY

| 2008-2009 Saturn VUE

| 2008-2009 HUMMER H2

This bulletin is being revised to update the DTCs that may be set in the SDM. Please discard Corporate Bulletin Number 08-09-41-002 (Section 09 - Restraints).

Important: This bulletin only applies to the DTC Symptom codes listed below.

Technicians may encounter an intermittent or current SIR indicator on the Instrument Panel Cluster (IPC) with DTC(s) B0012 04, 0E; B0013 04, 0E; B0016 04, 0E; B0019 04, 0E; B0020 04, 0E; B0022, B0023 04 0E; B0033 04, 0E; B0040 04, 0E; B0042 and B044 set in the sensing and diagnostic module (SDM).

This could be caused by a loose, missing, or broken Connector Position Assurance (CPA) retainer at the Air Bag for the set DTC.

If loose, remove the connector and reinstall correctly by first pushing the connector body in completely and then pushing in the CPA retainer completely. If the CPA is broken, missing or will not seat in the connector correctly, replace the CPA retainer with P/N 54590003 (Orange CPA) that is located in the SIR Repair Tray (J-38125-SIR) of the terminal repair kit.

If the CPA retainer P/N 54590003 (Orange CPA) cannot be located in the terminal repair kit, contact Kent Moore Tools @ 1-800-GM-TOOLS and order P/N 54590003-PKG to obtain a package of 5.