For 1990-2009 cars

## Heater Inlet Hose Replacement LNF

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling.
2. Remove the evaporator hose assembly. Refer to Air Conditioning Evaporator Hose Assembly Replacement
3. Remove the condenser tube. Refer to Condenser Tube Replacement

1 | Heater Inlet Hose

#### Procedure

Using J 38185 to reposition the heater inlet hose clamps.

#### Special Tools

J 38185 Hose Clamp Pliers