For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) retainer. Refer to Instrument Panel Retainer Replacement.
2. Remove the windshield defroster duct retaining screws.
3. Remove the windshield defroster duct.

### Installation Procedure

1. Install the windshield defroster duct.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the windshield defroster duct screws.

Tighten
Tighten the screws to 1.5 N·m (13 lb in).

3. Install the I/P retainer. Refer to Instrument Panel Retainer Replacement .