For 1990-2009 cars

### Removal Procedure

1. Remove the engine mount. Refer to Engine Mount Replacement .
2. Remove the engine mount bracket to engine bolts.
3. Remove the engine mount bracket.

### Installation Procedure

1. Position the engine mount bracket to the engine.
2. Install the engine mount bracket bolts in the following locations:

• | The long bolts in the forward and lower front holes

• | The short bolt in the upper rear hole

Notice: Refer to Fastener Notice in the Preface section.

3. Tighten the engine mount bracket bolts.

Tighten
Tighten the bolts in the sequence shown to 100 N·m (74 lb ft).

4. Install the engine mount. Refer to Engine Mount Replacement .