For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the interior trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector. Refer to Front Side Door Water Deflector Replacement .

1 | Front Side Door Lock Screw (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
2 | Front Side Door Lock Assembly