For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the steering column trim covers. Refer to Steering Column Trim Covers Replacement.

1 | Ignition and Start Switch Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Turn the ignition lock cylinder to the run position before removing the ignition and start switch bolts.

Tighten
2 N·m (18 lb in)

2 | Ignition and Start Switch

#### Procedure

Disconnect any electrical connectors as needed.