For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement.

1 | Drive Belt Tensioner

#### Procedure

1. Use the proper tool to rotate the drive belt tensioner.
2. Remove the drive belt from the pulleys and tensioner.

2 | Drive Belt

#### Procedure

1. Clean and inspect the drive belt surfaces of all the pulleys.
2. Inspect the drive belt for correct alignment.