For 1990-2009 cars

Table 1: | Indicators
Table 2: | Driver Information Center

#### Indicators

Symbol | Reference
--- | ---
| ABS: ABS Description and Operation
| Air Bag: SIR System Description and Operation
(Export) BRAKE | Brake: Hydraulic Brake System Description and Operation
| Charge: Charging System Description and Operation
| Engine Coolant Temperature: Cooling System Description and Operation
| Engine Oil Pressure: The IPC illuminates the engine oil pressure (EOP) indicator when the PCM/ECM detects the EOP is low from the EOP switch.
| Front Fog Lamps: Exterior Lighting Systems Description and Operation
| High Beam: Exterior Lighting Systems Description and Operation
| MIL: Engine Control Module Description for the 2.2L or 2.4L engine
| Seatbelt: Seat Belt System Description and Operation
| Security: Content Theft Deterrent (CTD) Description and Operation
| Traction Disabled: ABS Description and Operation
| Turn Signals: Exterior Lighting Systems Description and Operation
| Upshift Indicator: The Upshift indicator notifies the driver when to shift to a higher transmission range. The IPC illuminates the Upshift indicator as determined by the PCM/ECM.

#### Driver Information Center

Message | Reference
--- | ---
AUTO LIGHTS OFF | Exterior Lighting Systems Description and Operation
AUTO LIGHTS ON | Exterior Lighting Systems Description and Operation
BATTERY SAVER ACTIVE | Charging System Description and Operation
BRAKE FLUID | Hydraulic Brake System Description and Operation
CHARGING SYSTEM ACTIVE | Charging System Description and Operation
CHANGE OIL SOON | The DIC displays this message when the PCM/ECM determines that the engine oil life is less than a pre-determined value. Refer to GM Oil Life System Resetting
CHECK GAS CAP | Evaporative Emission Control System Description for the 2.0L engine or Evaporative Emission Control System Description for the 2.2L or 2.4L engine
CRUISE CONTROL ACTIVE | Cruise Control Description and Operation
DOOR AJAR | Power Door Locks Description and Operation
ENG PWR REDUCED | Cooling System Description and Operation
ICE POSSIBLE | The driver information center (DIC) displays this message when the outside air temperature drops below 2°C (36°F). When the temperature rises above 5.5°C (42°F), the message turns OFF.
KEY FOB BATT LOW | Keyless Entry System Description and Operation
LOW COOLANT | Cooling System Description and Operation
LOW FUEL | The DIC displays this message when the ECM/PCM detects that the fuel level is below a pre-determined value from the fuel level sensor.
LOW OIL LEVEL | The DIC displays this message when the PCM/ECM detects a low oil level condition.
LOW WASHER FLUID | Wiper/Washer System Description and Operation
LOW TRACTION | ABS Description and Operation
POWER STEERING | Power Steering System Description and Operation
PARKING BRAKE | Park Brake System Description and Operation
SERVICE AIR BAG | SIR System Description and Operation
SERVICE VEHICLE SOON | The driver information center (DIC) displays this message when the BCM or ECM/PCM detects certain vehicle malfunctions that are not emissions related.
STARTING DISABLED | Starting System Description and Operation
TRUNK AJAR | Luggage Compartment Description and Operation