For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the headliner. Refer to Headlining Trim Panel Replacement .

1 | Inflatable Restraint Roof Rail Module Screw Notice: Refer to Fastener Notice in the Preface section. Tighten 8 N·m (71 lb in)
2 | Inflatable Restraint Roof Rail Module Bolt Tighten 8 N·m (71 lb in)
3 | Inflatable Restraint Roof Rail Module Bolt Tighten 8 N·m (71 lb in)
4 | Inflatable Restraint Roof Rail Module Retainer (Qty: 3)
5 | Inflatable Restraint Roof Rail Module Bolt Tighten 8 N·m (71 lb in)
6 | Inflatable Restraint Roof Rail Module Assembly Tip

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connector.