For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position Assembly to Brake Bracket Bolt | 9 N·m | 80 lb in
Air Cleaner Assembly Nut | 10 N·m | 89 lb in
Air Cleaner Intake Duct Bolt | 10 N·m | 89 lb in
Air Cleaner Intake Duct Clamp | 5 N·m | 44 lb in
Air Cleaner Outlet Resonator Clamp | 5 N·m | 44 lb in
Camshaft Position (CMP) Sensor Bolt | 10 N·m | 89 lb in
Crankshaft Position (CKP) Sensor Bolt | 8 N·m | 71 lb in
Engine Control Module (ECM) Harness Connector Bolt | 4 N·m | 35 lb in
Engine Coolant Temperature (ECT) Sensor | 10 N·m | 89 lb in
EVAP Canister Bolt | 10 N·m | 89 lb in
EVAP Canister Purge Valve Bracket Nut | 18 N·m | 13 lb ft
Fuel Feed Pipe Bracket Nut | 10 N·m | 89 lb in
Fuel Fill Hose Clamp | 4.5 N·m | 40 lb in
Fuel Fill Pipe Lower Bolt | 10 N·m | 89 lb in
Fuel Filter Bracket Bolt | 10 N·m | 89 lb in
Fuel Rail Stud | 10 N·m | 89 lb in
Fuel Tank Strap Bolt | 25 N·m | 18 lb ft
Heated Oxygen Sensor (HO2S) - Position 1 | 30 N·m | 22 lb ft
Heated Oxygen Sensor (HO2S) - Position 2 | 41 N·m | 30 lb ft
Ignition Coil Bolt | 10 N·m | 89 lb in
Knock Sensor (KS) Bolt | 25 N·m | 18 lb ft
Mass Air Flow (MAF) Sensor Bolt | 0.6 N·m | 5 lb in
Rear Brake Hose Bracket Nut | 10 N·m | 89 lb in
Secondary Air Injection (AIR) Check Valve Bolt | 22 N·m | 16 lb ft
Secondary Air Injection (AIR) Pump Bolt | 20 N·m | 15 lb ft
Secondary Air Injection (AIR) Pump Outlet Hose Bracket Nut | 10 N·m | 89 lb in
Spark Plug | 20 N·m | 15 lb ft
Throttle Body Bolt | 10 N·m | 89 lb in