For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

Remove the fuel feed intermediate pipe. Refer to Fuel Feed Intermediate Pipe Replacement.

1 | Camshaft Position Sensor Bolt Caution: Refer to Fastener Caution in the Preface section. Tighten 10 N·m (89 lb in)
2 | Camshaft Position Sensor O-ring

#### Procedure

Lubricate the camshaft position sensor O-ring seal with clean engine oil.

3 | Camshaft Position Sensor

#### Procedure

1. Disconnect the sensor harness connector.
2. Inspect the camshaft position sensor for damage, replace as necessary.