For 1990-2009 cars

1. Lubricate the oil filter seal (84) with transmission fluid.

Caution: Gently tap the filter seal (84) evenly into the bore, to prevent damage to the case bore and seal.

2. Install a new oil filter seal (84) into the transmission case (51). You may use a large socket as an installer in order to tap on the seal.
3. Install a new filter assembly (85) into the filter seal (84). If necessary, twist the filter slightly during installation.