For 1990-2009 cars

## Inflatable Restraint Side Impact Sensor Replacement Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.
3. Reposition the water deflector.

1 | Side Impact Sensor Bolt (Qty: 2) Caution: Refer to Fastener Caution in the Preface section.

#### Procedure

Loosen the bolts in order to remove the sensor.

Tighten
8 N·m (71 lb in)

2 | Side Impact Sensor

#### Procedure

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connector.