For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Pedal Position Assembly Bolts | 9 N·m | 80 lb in
Air Cleaner Assembly Attaching Screws | 3 N·m | 27 lb in
Air Cleaner Assembly Bolts | 10 N·m | 89 lb in
Air Cleaner Intake Duct Assembly Bolt | 10 N·m | 89 lb in
Air Cleaner Intake Duct Clamp | 5 N·m | 44 lb in
BARO Sensor | 10 N·m | 89 lb in
Boost Control Solenoid Bolt | 10 N·m | 89 lb in
Bypass Vavle Actuator Bolt | 10 N·m | 89 lb in
CKP Sensor Stud | 22 N·m | 16 lb ft
Coolant Overflow Pipe | 8 N·m | 71 lb in
Engine Coolant Temperature (ECT) Sensor | 22 N·m | 16 lb ft
Engine Identification Cover Nuts | 10 N·m | 89 lb in
EVAP Canister Purge Valve Mounting Bracket Nut | 8 N·m | 71 lb in
EVAP Canister Retaining Bolt | 10 N·m | 89 lb in
Fuel Filler Hose Clamp | 4.5 N·m | 40 lb in
Fuel Filler Pipe Attaching Screw | 10 N·m | 89 lb in
Fuel Filler Pipe Lower Retaining Bolt | 10 N·m | 89 lb in
Fuel Filter Retaining Bolt | 10 N·m | 89 lb in
Fuel Rail Studs | 10 N·m | 89 lb in
Fuel Supply Line Fitting | 14 N·m | 10 lb ft
Fuel Tank Strap Bolts | 25 N·m | 18 lb ft
Heated Oxygen Sensor (HO2S) 1 | 30 N·m | 22 lb ft
Heated Oxygen Sensor (HO2S) 2 | 41 N·m | 30 lb ft
Ignition Coil Cover Screws | 8 N·m | 71 lb in
Intake Air Temperature (IAT) Sensor Bolt | 10 N·m | 89 lb in
Knock Sensor (KS) Bolt | 25 N·m | 18 lb ft
Manifold Absolute Pressure (MAP) Sensor Bolt | 10 N·m | 89 lb in
Mass Air Flow (MAF) Sensor Screws | 2 N·m | 18 lb in
Rear Brake Hose Bracket Nut | 10 N·m | 89 lb in
Spark Plugs | 20 N·m | 15 lb in
Throttle Body Attaching Bolts | 10 N·m | 89 lb in