For 1990-2009 cars

# Headliner Wet At Center Map Light/Sunroof Switch Area (Adjust Sunroof and Apply Lube)

Subject: | Headliner Wet At Center Map Light/Sunroof Switch Area (Adjust Sunroof and Apply Lube)

Models: | 2005-2008 Chevrolet Cobalt

| 2005-2006 Pontiac Pursuit (Canada Only)

| 2007-2008 Pontiac G5

| 2003-2007 Saturn ION

This bulletin is being revised to change the graphic in Step 7 and update the model years. Please discard Corporate Bulletin Number 06-08-67-019 (Section 08 - Body and Accessories).

### Condition

Some customers may comment that the headliner is wet or damp in front by the map light/sunroof switch.

### Cause

This condition may be caused by the sunroof being out of adjustment in the front. This causes water to get past the seal and wick though the conduit pipe, dripping on the map light /sunroof switch and the headliner.

### Correction

Adjust the sunroof following the procedure below.

1. Open the sunshade.
2. Close the sunroof glass.
3. Loosen the adjustment screws.
4. Adjust the front of the sunroof glass flush to 0.5 mm (0.02 in) above the roof panel. Tighten the screws.
5. Adjust the rear of the sunroof glass flush to 0.5 mm (0.02 in) above the roof panel. Tighten the screws.
6. Open the sunroof.
7. Apply Super Lube® to the sunroof cable where it enters the conduit pipe (as shown in the illustration above).
8. Return the sunroof and sunshade to the close position.

### Parts Information

Part Number | Description
--- | ---
12346241 (U.S.) 10953474 (Canada) | Super Lube®

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
B2720 | Panel, Sunroof - Align | Use Published Labor Operation Time