For 1990-2009 cars

## Inflatable Restraint Side Impact Sensor Replacement Sedan

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Reposition the water deflector.

1 | Side Impact Sensor Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Loosen the bolts in order to remove the sensor.

Tighten
8 N·m (71 lb in)

2 | Side Impact Sensor

#### Procedure

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connector.

## Inflatable Restraint Side Impact Sensor Replacement Coupe

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .
2. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
3. Reposition the water deflector.

1 | Side Impact Sensor Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

Loosen the bolts in order to remove the sensor.

Tighten
8 N·m (71 lb in)

2 | Side Impact Sensor

#### Procedure

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connector.