For 1990-2009 cars

### Removal Procedure

1. Remove the front seat. Refer to Front Seat Replacement - Bucket .
2. Remove the front carpet retainer.
3. Pull the carpet up to access the floor duct.
4. Unsnap the floor duct from the floor support beam. Disengage the floor duct from the center floor outlet duct and remove from the vehicle.

### Installation Procedure

1. Align the floor duct with the center floor outlet duct.
2. Align the floor duct with the floor support beam and snap into place.
3. Reposition the carpet.
4. Install the carpet retainer.
5. Install the front seat. Refer to Front Seat Replacement - Bucket .