For 1990-2009 cars

Callout | Component Name
--- | ---
Caution: Refer to SIR Inflator Module Handling and Storage Caution in the Preface section. Caution: Refer to SIR Caution in the Preface section.

#### Preliminary Procedures

Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling .

1 | Instrument Panel Trim Plate
2 | Instrument Panel Compartment Assembly Tip Squeeze the inner compartment sides together in order to lower the door past the down stops.
3 | Instrument Panel Compartment Accessory Hole Cover
4 | Instrument Panel Inflatable Restraint Module Bolt (Qty: 2) Notice: Refer to Fastener Notice in the Preface section. Tighten 10 N·m (89 lb in)
5 | Instrument Panel Inflatable Restraint Module Tip

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connector.
3. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required period. Refer to Inflator Module Handling and Scrapping .