For 1990-2009 cars

1. Adjust the rear compartment lid fore-aft and cross-car by loosening the hinge to compartment lid nuts (1). Position the rear compartment lid as needed.
2. Adjust the front of the compartment lid up and down by loosening hinge to quarter panel bolts (2). Position the rear compartment lid as needed.
3. Adjust the rear of the compartment lid by adjusting the lock striker up and down.

Notice: Refer to Fastener Notice in the Preface section.

4. Tighten the rear compartment lid hinge to compartment lid nuts (1).

Tighten
Tighten the nuts to 10 N·m (89 lb in).

5. Tighten the rear compartment lid hinge to quarter panel bolts (2).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

6. Tighten the latch striker bolts when the adjustments are complete.

Tighten
Tighten the bolts to 10 N·m (89 lb in).