For 1990-2009 cars

1. Install the 1-2 shift valve spring (301), the 1-2 shift valve (302), the 1-2 shift solenoid (305) with O-ring (303) and the 1-2 shift solenoid retainer clip (304).
2. Install the 2-3 shift valve spring (306), the 2-3 shift valve (307), the 2-3 shift solenoid (305) with O-ring (303) and the 2-3 shift solenoid retainer clip (304).
3. Install the torque signal regulator spring (308), the torque signal regulator valve (309), the Pressure Control Solenoid (PCS) with two O-rings and screen (312, 309, 310) and the PCS retainer clip (304).
4. Install the actuator oil filter (314), with the O-ring (313) and the actuator oil filter retainer clip (304).
5. Install the actuator feed limit valve (315), the actuator feed limit spring (316), the bore plug (317) and the actuator feed limit valve retainer clip (304).
6. Install the 3-4 shift valve spring (318), the 3-4 shift valve (319), the bore plug (321), with O-ring (320) and the 3-4 shift valve retainer clip (304).
7. Install the accumulator valve (323), the plug (341) and the 1-2/3-4 accumulator valve retainer clip (304).
8. Install the pressure regulator valve (328), the pressure regulator valve spring (327), the isolator spring (326), the pressure regulator boost valve (325), the bushing (324) and the pressure regulator valve retainer clip (304).
9. Install the TCC control valve (334), the spring (333), the bore plug (317) and the TCC control valve retainer clip (304).
10. Install the spring (340), the TCC regulated apply valve (339), the TCC solenoid (335) with two O-rings (337 and 338) and screen, and the TCC solenoid retainer clip (304).