For 1990-2009 cars

Connector 1: | X100 Engine Harness to the Transmission Harness (MN5/MX0)
Connector 2: | X101 Engine Harness to the Body Harness (L61/LE5)
Connector 3: | X102 Engine Harness to the Crankshaft Position Jumper (LNF)
Connector 4: | X110 Forward Lamp Harness to the Right Headlamp Assembly
Connector 5: | X111 Forward Lamp Harness to the Left Headlamp Assembly
Connector 6: | X121 Forward Lamp Harness to the Body Harness
Connector 7: | X160 Engine Harness to the Fuel Injector Harness (L61/LE5)
Connector 8: | X161 Engine Harness to the Body Harness (LNF)
Connector 9: | X162 Engine Harness to the Fuel Injector Harness (LNF)
Connector 10: | X170 Body Harness to the Right Front WSS Harness (JM4/JL4/JL9)
Connector 11: | X171 Body Harness to the Left Front WSS Harness (JM4/JL4/JL9)
Connector 12: | X200 I/P Harness to the Body Harness
Connector 13: | X201 I/P Harness to the Body Harness
Connector 14: | X202 Body Harness to the Passenger Inflatable Restraint I/P Module Harness (Cobalt Coupe)
Connector 15: | X202 Body Harness to the Passenger Inflatable Restraint I/P Module Harness (Cobalt Sedan/Pontiac G5)
Connector 16: | X210 I/P Harness to the HVAC Harness
Connector 17: | X275 I/P Harness to the SIR Coil Assembly
Connector 18: | X302 Headliner Harness to Sun Roof Control Module
Connector 19: | X305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness
Connector 20: | X307 Body Harness to A/T Shift Control Module (MN5/MX0)
Connector 21: | X314 Body Harness to the Passenger Seat Harness (KA1)
Connector 22: | X315 Body Harness to the Driver Seat Harness (KA1)
Connector 23: | X316 Body Harness to the Passenger Seat Harness
Connector 24: | X319 Body Harness to Left Roof Rail Module Harness (ASF)
Connector 25: | X320 Body Harness to Right Roof Rail Module Harness (ASF)
Connector 26: | X321 Body Harness to the Headliner Harness (UE1)
Connector 27: | X321 Body Harness to the Headliner Harness (without UE1)
Connector 28: | X400 Battery Cable to the Body Harness
Connector 29: | X401 Body Harness to the Rear Compartment Lamp Harness
Connector 30: | X492 Body Harness to the Left Rear Tail Lamp Assembly Harness (Sedan)
Connector 31: | X493 Body Harness to the Right Rear Tail Lamp Assembly Harness (Sedan)
Connector 32: | X494 License and Backup Lamp Harness to the Body Harness (G5)
Connector 33: | X495 License Lamp Harness to Right Backup Lamp Assembly (G5)
Connector 34: | X496 License Lamp Harness to Left Backup Lamp Assembly (G5)
Connector 35: | X497 License Lamp Harness to License Lamp Assembly (G5)
Connector 36: | X500 Body Harness to the Driver Door Harness (AU3/DG7)
Connector 37: | X500 Body Harness to the Left Front Door Harness (without AU3/DG7)
Connector 38: | X600 Body Harness to the Passenger Door Harness (AU3/DG7)
Connector 39: | X600 Body Harness to the Right Front Door Harness (without AU3/DG7)
Connector 40: | X700 Body Harness to the Left Rear Door Harness (Sedan with AU3/DG7)
Connector 41: | X800 Body Harness to the Right Rear Door Harness (Sedan with AU3/DG7)

### X100 Engine Harness to the Transmission Harness (MN5/MX0)

#### Connector Part Information

- OEM: 15472125
- Service: 15305857
- Description: 14-Way F Micro-Pack 100W Series Sealed (BK)

#### Connector Part Information

- OEM: 15443076
- Service: 12160782
- Description: 20-Way M Micro-Pack 100W Series Sealed (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X100 Engine Harness to the Transmission Harness (MN5/MX0)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 L-GN | 1222 | 1-2 Shift Solenoid Valve Control | A | 0.35 L-GN | 1222 | 1-2 Shift Solenoid Valve Control
B | 0.35 YE/BK | 1223 | 2-3 Shift Solenoid Valve Control | B | 0.35 YE/BK | 1223 | 2-3 Shift Solenoid Valve Control
C | 0.35 OG/BK | 1228 | PC Solenoid Valve High Control (Sol. A) | C | 0.35 OG/BK | 1228 | PC Solenoid Valve High Control (Sol. A)
D | 0.35 L-BU/WH | 1229 | PC Solenoid Valve Low Control (Sol. A) | D | 0.35 L-BU/WH | 1229 | PC Solenoid Valve Low Control (Sol. A)
E | 0.35 PK | 1039 | Ignition 1 Voltage | E | 0.35 PK | 839 | Ignition 1 Voltage
F-K | -- | -- | Not Used | F-K | -- | -- | Not Used
L | 0.35 YE/BK | 1227 | TFT Sensor Signal | L | 0.35 YE/BK | 1227 | TFT Sensor Signal
M | 0.35 TN | 2762 | Low Reference | M | 0.35 TN | 452 | Low Reference
N | -- | -- | Not Used | N | -- | -- | Not Used
P | 0.35 OG | 1226 | Transmission Fluid Pressure Switch Signal C | P | 0.35 OG | 1226 | Transmission Fluid Pressure Switch Signal C
R | 0.35 D-BU | 1225 | Transmission Fluid Pressure Switch Signal B | R | 0.35 D-BU | 1225 | Transmission Fluid Pressure Switch Signal B
S | 0.35 OG/BK | 1230 | AT ISS High Signal | S | 0.35 OG/BK | 1230 | AT ISS High Signal
T | 0.35 TN/BK | 422 | TCC Solenoid Valve Control | T | 0.35 TN/BK | 418 | TCC Solenoid Valve Control
U | 0.35 YE | 657 | TCC Release Switch Signal | U | 0.35 YE | 1804 | TCC Release Switch Signal
V | 0.35 D-BU/WH | 1231 | AT ISS Low Signal | V | 0.35 D-BU/WH | 1231 | AT ISS Low Signal
W | -- | -- | Not Used | W | -- | -- | Not Used

### X101 Engine Harness to the Body Harness (L61/LE5)

#### Connector Part Information

- OEM: 15326861
- Service: 15306396
- Description: 14-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326856
- Service: 15326820
- Description: 14-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: 15326269/19
- Core/Insulation Crimp: E/4
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X101 Engine Harness to the Body Harness (L61/LE5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | A | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
B | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus- | B | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
C | 0.5 L-GN | 24 | Backup Lamp Supply Voltage (M86/MN5) | C | 0.5 L-GN | 24 | Backup Lamp Supply Voltage (M86/MN5)
D | 0.35 BN | 4 | Accessory Voltage (MN5/MX0) | D | 0.35 BN | 4 | Accessory Voltage (MN5/MX0)
E | 0.35 D-GN | 335 | Cooling Fan Relay Control | E | 0.35 D-GN | 335 | Cooling Fan Relay Control
F | 0.35 D-GN | 6307 | PNP Switch Signal (MN5) | F | 0.35 D-GN | 6307 | PNP Switch Signal (MN5)
G | 0.35 BN/WH | 6354 | Transmission Output Speed Sensor Signal (M86) | G | 0.35 BN/WH | 6354 | Transmission Output Speed Sensor Signal (M86)
H | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | H | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
J | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus- | J | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus-
K | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal (C67) | K | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal (C67)
L | 0.35 BN | 436 | Air Pump Relay Control (NU3) | L | 0.35 BN | 436 | Air Pump Relay Control (NU3)
M | 0.35 L-BU | 6289 | Air Temperature Sensor Signal | M | 0.35 L-BU | 6289 | Air Temperature Sensor Signal
N | 0.35 YE | 492 | MASS Air Flow Sensor Signal | N | 0.35 YE | 492 | MASS Air Flow Sensor Signal
P | 0.35 PU/WH | 6356 | Transmission Output Speed Sensor - Low Reference (M86) | P | 0.35 PU/WH | 6356 | Transmission Output Speed Sensor - Low Reference (M86)

### X102 Engine Harness to the Crankshaft Position Jumper (LNF)

#### Connector Part Information

- OEM: 15326808
- Service: See Catalog
- Description: 3-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326813
- Service: See Catalog
- Description: 3-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X102 Engine Harness to the Crankshaft Position Jumper (LNF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 2867 | Crankshaft Position Sensor Supply Voltage | A | 0.5 L-GN | 2867 | Crankshaft Position Sensor Supply Voltage
B | 0.5 PU | 574 | Low Reference | B | 0.5 PU | 574 | Low Reference
C | 0.5 YE | 573 | CKP Sensor 1 Signal | C | 0.5 YE | 573 | CKP Sensor 1 Signal

### X110 Forward Lamp Harness to the Right Headlamp Assembly

#### Connector Part Information

- OEM: 12052848
- Service: 12101854
- Description: 6-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052849
- Service: 12101852
- Description: 6-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X110 Forward Lamp Harness to the Right Headlamp Assembly

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BK | 250 | Ground | A | 0.35 BK | 250 | Ground
B | 0.5 D-BU | 15 | Right Turn Signal Lamp Supply Voltage | B | 0.5 L-BU | 15 | Right Turn Signal Lamp Supply Voltage
C | 0.5 BN | 9 | Park Lamp Supply Voltage | C | 0.5 BN | 9 | Park Lamp Supply Voltage
D | 0.8 TN/WH | 312 | Right Headlamp Low Beam Supply Voltage | D | 0.8 OG | 312 | Right Headlamp Low Beam Supply Voltage
E | 0.5 L-GN/BK | 311 | Right Headlamp High Beam Supply Voltage | E | 0.5 PK | 311 | Right Headlamp High Beam Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

### X111 Forward Lamp Harness to the Left Headlamp Assembly

#### Connector Part Information

- OEM: 12052848
- Service: 12101854
- Description: 6-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052849
- Service: 12101852
- Description: 6-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12048074/2
- Core/Insulation Crimp: E/1
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X111 Forward Lamp Harness to the Left Headlamp Assembly

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 150 | Ground | A | 0.5 BK | 150 | Ground
B | 0.5 L-BU | 14 | Left Turn Signal Lamp Supply Voltage | B | 0.8 L-BU | 14 | Left Turn Signal Lamp Supply Voltage
C | 0.5 BN | 9 | Park Lamp Supply Voltage | C | 0.5 BN | 9 | Park Lamp Supply Voltage
D | 0.5 YE | 712 | Left Headlamp Low Beam Supply Voltage | D | 0.5 OG | 712 | Left Headlamp Low Beam Supply Voltage
E | 0.5 D-GN/WH | 711 | Left Headlamp High Beam Supply Voltage | E | 0.8 PK | 711 | Left Headlamp High Beam Supply Voltage
F | -- | -- | Not Used | F | -- | -- | Not Used

### X121 Forward Lamp Harness to the Body Harness

#### Connector Part Information

- OEM: 15326829
- Service: 88988924
- Description: 6-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326833
- Service: 15326833
- Description: 6-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

#### X121 Forward Lamp Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 YE | 1834 | Forward Discriminating Sensor Signal | A | 0.35 YE | 1834 | Forward Discriminating Sensor Signal
B | 0.35 TN/OG | 5045 | Discriminating Sensor - Low Reference | B | 0.35 TN/OG | 5045 | Discriminating Sensor - Low Reference
C | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal | C | 0.35 D-GN/WH | 636 | Ambient Air Temperature Sensor Signal
D | 0.35 YE/BK | 61 | Low Reference | D | 0.35 YE/BK | 61 | Low Reference
E | 0.35 PK/BK | 109 | Hood Ajar Switch Signal (AP3) | E | 0.35 PK/BK | 109 | Hood Ajar Switch Signal (AP3)
F | 0.35 PU | 5531 | Hood Closed Switch Signal (AP3) | F | 0.35 PU | 5531 | Hood Closed Switch Signal (AP3)

### X160 Engine Harness to the Fuel Injector Harness (L61/LE5)

#### Connector Part Information

- OEM: 15326836
- Service: 88986255
- Description: 8-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326839
- Service: See Catalog
- Description: 8-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X160 Engine Harness to the Fuel Injector Harness (L61/LE5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 TN | 1744 | Fuel Injector 1 Control | A | 0.5 BK | 1744 | Fuel Injector 1 Control
B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control | B | 0.5 L-GN/BK | 1745 | Fuel Injector 2 Control
C | 0.5 PK/BK | 1746 | Fuel Injector 3 Control | C | 0.5 PK/BK | 1746 | Fuel Injector 3 Control
D | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control | D | 0.5 L-BU/BK | 844 | Fuel Injector 4 Control
E | 0.5 PK/BK | 5292 | Ignition 1 Voltage | E | 0.5 PK | 139 | Ignition 1 Voltage
F | 0.35 OG/BK | 469 | Low Reference | F | 0.5 OG/BK | 469 | Low Reference
G | 0.35 L-GN | 432 | MAP Sensor Signal | G | 0.5 L-GN | 432 | MAP Sensor Signal
H | 0.35 GY | 2704 | 5-Volt Reference (L61, LE5 with M86) | H | 0.35 GY | 2704 | 5-Volt Reference
0.35 PU/WH | 5-Volt Reference (LE5 with MN5)

### X161 Engine Harness to the Body Harness (LNF)

#### Connector Part Information

- OEM: 15326084
- Service: See Catalog
- Description: 16-Way F GT 150 280 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326085
- Service: See Catalog
- Description: 16-Way M GT 150 280 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X161 Engine Harness to the Body Harness (LNF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 GY/WH | 3122 | HO2S Heater Low Control | A | 0.5 GY/WH | 3122 | HO2S Heater Low Control
B | 0.35 BN/WH | 419 | MIL Control | B | 0.35 BN/WH | 419 | MIL Control
C | 0.35 D-GN | 335 | Low Speed Cooling Fan Relay Control | C | 0.35 D-GN | 335 | Low Speed Cooling Fan Relay Control
D | 0.35 TN | 891 | Boost Gauge Signal | D | 0.35 TN | 891 | Boost Gauge Signal
E | 0.35 GY | 2700 | 5-Volt Reference | E | 0.35 GY | 2700 | 5-Volt Reference
F | 0.5 TN | 5514 | Low Reference | F | 0.5 TN | 5514 | Low Reference
G | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal | G | 0.35 OG/BK | 380 | A/C Refrigerant Pressure Sensor Signal
H | 2 BK/WH | 451 | Ground | H | 2 BK/WH | 451 | Ground
J | 0.35 YE | 492 | MASS Air Flow Sensor Signal | J | 0.35 YE | 492 | MASS Air Flow Sensor Signal
K | 0.5 PU | 3120 | HO2S High Signal | K | 0.5 PU | 3120 | HO2S High Signal
L | 0.5 TN/WH | 3121 | HO2S Low Signal | L | 0.5 TN/WH | 3121 | HO2S Low Signal
M | 0.5 YE | 400 | VSS High Signal | M | 0.5 YE | 400 | VSS High Signal
N | 0.5 PU | 401 | VSS Low Signal | N | 0.5 PU | 401 | VSS Low Signal
P | 0.35 TN | 2760 | Low Reference | P | 0.35 TN | 2760 | Low Reference
R | 0.35 L-BU | 6289 | MAF/IAT Sensor Signal | R | 0.35 L-BU | 6289 | MAF/IAT Sensor Signal
S | 0.5 L-GN | 24 | Backup Lamp Supply Voltage | S | 0.5 L-GN | 24 | Backup Lamp Supply Voltage

### X162 Engine Harness to the Fuel Injector Harness (LNF)

#### Connector Part Information

- OEM: 33472-1216
- Service: See Catalog
- Description: 12-Way F MX 150 Series (BK)

#### Connector Part Information

- OEM: 33482-1206
- Service: See Catalog
- Description: 12-Way M (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X162 Engine Harness to the Fuel Injector Harness (LNF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
1 | 1 BN | 4801 | Fuel Injector High Voltage Control Cylinder 1 | 1 | 1 BN | 4801 | Fuel Injector High Voltage Control Cylinder 1
2 | 1 D-BU | 4802 | Fuel Injector High Voltage Control Cylinder 2 | 2 | 1 D-BU | 4802 | Fuel Injector High Voltage Control Cylinder 2
3 | 1 D-GN | 4803 | Fuel Injector High Voltage Control Cylinder 3 | 3 | 1 D-GN | 4803 | Fuel Injector High Voltage Control Cylinder 3
4 | 1 L-BU | 4804 | Fuel Injector High Voltage Control Cylinder 4 | 4 | 1 L-BU | 4804 | Fuel Injector High Voltage Control Cylinder 4
5 | 0.5 TN | 808 | Low Reference | 5 | 0.5 TN | 808 | Low Reference
6 | -- | -- | Not Available | 6 | -- | -- | Not Available
7 | 1 BN/WH | 4901 | Fuel Injector High Voltage Supply Cylinder 1 | 7 | 1 BN/WH | 4901 | Fuel Injector High Voltage Supply Cylinder 1
8 | 1 D-BU/WH | 4902 | Fuel Injector High Voltage Supply Cylinder 2 | 8 | 1 D-BU/WH | 4902 | Fuel Injector High Voltage Supply Cylinder 2
9 | 1 D-GN/WH | 4903 | Fuel Injector High Voltage Supply Cylinder 3 | 9 | 1 D-GN/WH | 4903 | Fuel Injector High Voltage Supply Cylinder 3
10 | 1 L-BU/WH | 4904 | Fuel Injector High Voltage Supply Cylinder 4 | 10 | 1 L-BU/WH | 4904 | Fuel Injector High Voltage Supply Cylinder 4
11 | 0.5 GY | 598 | 5-Volt Reference | 11 | 0.5 GY | 598 | 5-Volt Reference
12 | 0.5 YE | 2918 | FRP Sensor Signal | 12 | 0.5 YE | 2918 | FRP Sensor Signal

### X170 Body Harness to the Right Front WSS Harness (JM4/JL4/JL9)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X170 Body Harness to the Right Front WSS Harness (JM4/JL4/JL9)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal | A | 0.5 D-GN | 872 | Right Front Wheel Speed Sensor Signal
B | 0.5 TN | 833 | Right Front Wheel Speed Sensor Low Reference | B | 0.5 TN | 833 | Right Front Wheel Speed Sensor Low Reference

### X171 Body Harness to the Left Front WSS Harness (JM4/JL4/JL9)

#### Connector Part Information

- OEM: 15326801
- Service: 15306156
- Description: 2-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326806
- Service: 15306166
- Description: 2-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X171 Body Harness to the Left Front WSS Harness (JM4/JL4/JL9)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-BU | 830 | Left Front Wheel Speed Sensor Signal | A | 0.5 D-GN | 830 | Left Front Wheel Speed Sensor Signal
B | 0.5 YE | 873 | Left Front Wheel Speed Sensor Low Reference | B | 0.5 TN | 873 | Left Front Wheel Speed Sensor Low Reference

### X200 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15336219
- Service: 15336219
- Description: 16-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15336224
- Service: 15336224
- Description: 16-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Pins: B, E-G, K-M
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins E-G: C/A
- Core/Insulation Crimp: Pins B, K, L: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, H, J
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins H: 2/A
- Core/Insulation Crimp: Pins: A, J: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: B-F, G, K-M
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins G: 2/4
- Core/Insulation Crimp: Pins E, F: E/4
- Core/Insulation Crimp: Pins B, K-M: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A, H, J
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X200 I/P Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 PK/BK | 1503 | Passenger Heated Seat High/Low Signal (KA1) | A | 0.35 PK/BK | 1503 | Passenger Heated Seat High/Low Signal (KA1)
B | 0.35 L-BU/BK | 1505 | Passenger Heated Seat Switch Signal (KA1) | B | 0.35 L-BU/BK | 1505 | Passenger Heated Seat Switch Signal (KA1)
C-D | -- | -- | Not Used | C-D | -- | -- | Not Used
E | 0.5 L-GN | 200 | Right Front Speaker Output (+) | E | 0.5 L-GN/BK | 200 | Right Front Speaker Output (+) (UQ3)
0.35 L-GN | 200 | Right Front Speaker (+) Output (UQ4)
F | 0.5 D-GN | 117 | Right Front Speaker Output (-) | F | 0.5 D-GN/BK | 117 | Right Front Speaker Output (-) (UQ3)
0.35 D-GN | 117 | Right Front Speaker Output (-) (UQ4)
G | 0.8 L-BU/BK | 115 | Right Rear Speaker Output (-) (UQ3) | G | 1 L-BU/BK | 115 | Right Rear Speaker Output (-) (UQ3)
0.8 L-BU | 115 | Right Rear Speaker Output (-) (UQ4) | 0.5 L-BU | 115 | Right Rear Speaker Output (-) (UQ4)
H | 0.8 D-BU | 46 | Right Rear Speaker Output (+) | H | 1 D-BU/BK | 46 | Right Rear Speaker Output (+) (UQ3)
0.5 D-BU | 46 | Right Rear Speaker Output (+) (UQ4)
J | BARE | 814 | Drain Wire (U2K) | J | BARE | 814 | Drain Wire (U2K)
K | 0.35 BN/WH | 367 | Left Audio Signal (+) (U2K) | K | 0.35 BN/WH | 367 | Left Audio Signal (+) (U2K)
L | 0.35 D-GN/WH | 368 | Right Audio Signal (+) (U2K) | L | 0.35 D-GN/WH | 368 | Right Audio Signal (+) (U2K)
M | 0.35 TN/WH | 372 | Audio Common (U2K) | M | 0.35 TN/WH | 372 | Audio Common (U2K)
N | 0.35 PK/BK | 2062 | Cellular Telephone Voice Signal (UE1) | N | 0.35 PK/BK | 2062 | Cellular Telephone Voice Signal (UE1)
P | 0.35 OG/BK | 2061 | Cellular Telephone Voice Low Reference (UE1) | P | 0.35 OG/BK | 2061 | Cellular Telephone Voice Low Reference (UE1)
R | 0.35 BARE | 813 | Drain Wire (UE1) | R | 0.35 BARE | 813 | Drain Wire (UE1)
S | -- | -- | Not Used | S | -- | -- | Not Used

### X201 I/P Harness to the Body Harness

#### Connector Part Information

- OEM: 15448129
- Service: 89046969
- Description: 40-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15475869
- Service: 88988307
- Description: 40-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Pins: A1, A2, A7, B1-B11, C1-C6, C8-C12, D1, D7, D8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins B7, B10, D7: C/A
- Core/Insulation Crimp: Pins A1, A2, A7, B1-B6, B8, B9, B11, C1-C6, C8-C12, D1, D8: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A3, A5, A6, D3, D6
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins D: 62/A
- Core/Insulation Crimp: Pins A3, A5, A6, D3: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1, A2, A7, B1-B11, C1-C6, C8-C12, D1, D7, D8
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins B7, B10, C11, C12, D7: 2/4
- Core/Insulation Crimp: Pins B6, B9, C3, C5, C6, D1, D8: E/4
- Core/Insulation Crimp: Pins A1, A2, A7, B1-B5, B8, B11, C1, C2, C4, C8-C10: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A3, A5, A6, D3, D4
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: D6
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: 2/A
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X201 I/P Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 L-BU | 1162 | APP Sensor 2 Signal | A1 | 0.35 L-BU | 1162 | APP Sensor 2 Signal
A2 | 0.35 D-BU | 1161 | APP Sensor 1 Signal | A2 | 0.35 D-BU | 1161 | APP Sensor 1 Signal
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | 0.35 PK | 353 | I/P Module Suppression Indicator Control | A4 | 0.35 PK | 353 | I/P Module Suppression Indicator Control
A5 | 0.5 GY | 118 | Left Front Speaker Output (-) | A5 | 0.35 GY | 118 | Left Front Speaker Output (-) (UQ4)
0.5 GY/BK | 118 | Left Front Speaker Output (-) (UQ3)
A6 | 0.35 PK | 339 | Ignition 1 Voltage (KA1) | A6 | 0.35 PK | 339 | Ignition 1 Voltage
0.35 PK | 339 | Ignition 1 Voltage (KA1)
A7 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data | A7 | 0.35 D-GN | 5060 | Low Speed GMLAN Serial Data
A8 | 0.35 OG/BK | 556 | Steering Wheel Position Sensor Low Reference (JL4/JL9) | A8 | 0.5 OG/BK | 556 | Steering Wheel Position Sensor Low Reference (JL4/JL9)
B1 | 0.35 PU | 1272 | Low Reference | B1 | 0.35 PU | 1272 | Low Reference
B2 | 0.35 BN | 1271 | Low Reference | B2 | 0.35 BN | 1271 | Low Reference
B3-B4 | -- | -- | Not Used | B3-B4 | -- | -- | Not Used
B5 | 0.35 D-BU/WH | 7361 | Clutch Pedal Position Sensor Supply Voltage (M86) | B5 | 0.35 D-BU/WH | 7361 | Clutch Pedal Position Sensor Supply Voltage (M86)
-- | Not Used (MN5/MX0) | -- | Not Used (MN5/MX0)
0.5 GY | 2709 | 5-Volt Reference (MU3) | 0.5 GY | 2709 | 5-Volt Reference (MU3)
B6 | 0.35 OG/BK | 7360 | Clutch Pedal Position Sensor Return (M86) | B6 | 0.35 L-GN | 7360 | Clutch Pedal Position Sensor Return (M86)
-- | Not Used (MN5/MX0) | -- | Not Used (MN5/MX0)
0.5 TN | 2759 | Low Reference (MU3) | 0.5 TN | 2759 | Low Reference (MU3)
B7 | 0.35 L-GN | 6338 | Clutch Pedal Position Sensor Signal (M86/MU3) | B7 | 0.35 L-GN | 6338 | Clutch Pedal Position Sensor Signal (M86/MU3)
-- | Not Used (MN5/MX0) | -- | Not Used (MN5/MX0)
B8 | 0.35 TN | 1274 | 5-Volt Reference | B8 | 0.35 TN | 1274 | 5-Volt Reference
B9 | 0.35 TN/BK | 723 | SIR Enable Signal - Passenger | B9 | 0.35 TN/BK | 723 | SIR Enable Signal - Passenger
B10 | 0.5 D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal (MN5/MX0) | B10 | 0.5 D-GN/WH | 1932 | Ignition Lock Cylinder Control Actuator Signal (MN5/MX0)
B11 | 0.35 WH/BK | 1164 | 5-Volt Reference | B11 | 0.35 WH/BK | 1164 | 5-Volt Reference
B12 | 0.35 TN | 891 | Boost Gage Signal (LNF) | B12 | 0.35 TN | 891 | Boost Gage Signal (LNF)
C1 | 0.35 PK | 1501 | Driver Heated Seat High/Low Signal (KA1) | C1 | 0.35 PK | 1501 | Driver Heated Seat High/Low Signal (KA1)
C2 | 0.8 L-GN/BK | 1794 | Rear Subwoofer Speaker Output (-) (UQ3) | C2 | 0.8 L-GN/BK | 1794 | Rear Subwoofer Speaker Output (-) (UQ3)
C3 | 0.8 D-BU/WH | 346 | Rear Subwoofer Speaker Output (+) (UQ3) | C3 | 0.8 D-BU/WH | 346 | Rear Subwoofer Speaker Output (+) (UQ3)
C4 | 0.35 L-BU | 1462 | Heated Seat Switch Signal (KA1) | C4 | 0.35 L-BU | 1462 | Heated Seat Switch Signal (KA1)
C5 | 0.35 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+ | C5 | 0.5 TN/BK | 2500 | High Speed GMLAN Serial Data Bus+
C6 | 0.35 TN | 2501 | High Speed GMLAN Serial Data Bus- | C6 | 0.5 TN | 2501 | High Speed GMLAN Serial Data Bus-
C7 | 0.35 L-BU | 1788 | Traction Control Switch Signal (JL4/JL9) | C7 | 0.35 L-BU | 1788 | Traction Control Switch Signal (JL4/JL9)
C8 | 0.35 BN/WH | 419 | MIL Control | C8 | 0.35 BN/WH | 419 | MIL Control
C9 | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal | C9 | 0.35 L-GN | 1715 | Windshield Wiper Switch High Signal
C10 | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control | C10 | 0.35 PK/WH | 1970 | Headlamp Low Beam Relay Control
C11 | 0.5 YE/BK | 116 | Left Rear Speaker Output (-) | C11 | 0.5 YE | 116 | Left Rear Speaker Output (-) (UQ4)
1 YE/BK | 116 | Left Rear Speaker Output (-) (UQ3)
C12 | 0.5 BN | 199 | Left Rear Speaker Output (+) | C12 | 0.5 BN | 199 | Left Rear Speaker Output (+) (UQ4)
0.8 BN/WH | 199 | Left Rear Speaker Output (+) (UQ3)
D1 | 0.5 TN | 201 | Left Front Speaker Output (+) | D1 | 0.5 TN/BK | 201 | Left Front Speaker Output (+) (UQ3)
0.5 TN | 201 | Left Front Speaker Output (+) (UQ4)
D2 | 0.35 GY | 1056 | 5-Volt Reference (JL4/JL9) | D2 | 0.5 GY | 1056 | 5-Volt Reference (JL4/JL9)
D3 | 0.8 RD/WH | 40 | Battery Positive Voltage | D3 | 0.8 RD/WH | 40 | Battery Positive Voltage
0.8 RD/WH | 40 | Battery Positive Voltage
D4 | 0.5 RD/WH | 240 | Battery Positive Voltage | D4 | 0.5 RD/WH | 240 | Battery Positive Voltage
D5 | 0.5 PK/BK | 6434 | CAN Bus High Serial Data (JL4/JL9) | D5 | 0.5 PK/BK | 6434 | CAN Bus High Serial Data (JL4/JL9)
0.5 YE | 6434 | CAN Bus High Serial Data (JL4/JL9)
D6 | 0.5 GY/BK | 6435 | CAN Bus Low Serial Data (JL4/JL9) | D6 | 0.5 GY/BK | 6435 | CAN Bus Low Serial Data (JL4/JL9)
0.5 GY/BK | 6435 | CAN Bus Low Serial Data (JL4/JL9)
D7 | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+) (UQ3) | D7 | 0.8 D-GN | 1795 | Right Subwoofer Speaker Output (+) (UQ3)
D8 | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-) (UQ3) | D8 | 0.8 L-BU/BK | 315 | Right Subwoofer Speaker Output (-) (UQ3)

### X202 Body Harness to the Passenger Inflatable Restraint I/P Module Harness (Cobalt Coupe)

#### Connector Part Information

- OEM: 15424636
- Service: 15306363
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15424638
- Service: 15306183
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X202 Body Harness to the Passenger Inflatable Restraint I/P Module Harness (Cobalt Coupe)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 L-GN/OG | 3024 | I/P Module Stage 1 Low Control | A1 | 0.35 OG | 3024 | I/P Module Stage 1 Low Control
A2 | 0.35 RD/WH | 3025 | I/P Module Stage 1 High Control | A2 | 0.35 YE | 3025 | I/P Module Stage 1 High Control
B1 | 0.35 PK/BK | 3026 | I/P Module Stage 2 Low Control | B1 | 0.35 PU | 3026 | I/P Module Stage 2 Low Control
B2 | 0.35 L-BU/OG | 3027 | I/P Module Stage 2 High Control | B2 | 0.35 GY | 3027 | I/P Module Stage 2 High Control

### X202 Body Harness to the Passenger Inflatable Restraint I/P Module Harness (Cobalt Sedan/Pontiac G5)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336477
- Service: 15306183
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X202 Body Harness to the Passenger Inflatable Restraint I/P Module Harness (Cobalt Sedan/Pontiac G5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 OG | 3024 | I/P Module Stage 1 Low Control | A1 | 0.35 OG | 3024 | I/P Module Stage 1 Low Control
A2 | 0.5 YE | 3025 | I/P Module Stage 1 High Control | A2 | 0.35 YE | 3025 | I/P Module Stage 1 High Control
B1 | 0.5 PU | 3026 | I/P Module Stage 2 Low Control | B1 | 0.35 PU | 3026 | I/P Module Stage 2 Low Control
B2 | 0.5 GY | 3027 | I/P Module Stage 2 High Control | B2 | 0.35 GY | 3027 | I/P Module Stage 2 High Control

### X210 I/P Harness to the HVAC Harness

#### Connector Part Information

- OEM: 15326870
- Service: 88953160
- Description: 2-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326874
- Service: 15306379
- Description: 2-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X210 I/P Harness to the HVAC Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 BK | 550 | Ground | A | 3 BK | 550 | Ground
B | 3 BN | 141 | Ignition 3 Voltage | B | 3 BN | 141 | Ignition 3 Voltage

### X275 I/P Harness to the SIR Coil Assembly

#### Connector Part Information

- OEM: 15479525
- Service: 15306186
- Description: 4-Way F Metri-Pack 280 Series (YE)

#### Connector Part Information

- OEM: 15336476
- Service: 15306363
- Description: 4-Way M Metri-Pack 280 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X275 I/P Harness to the SIR Coil Assembly

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control | A1 | 0.5 BN | 3020 | Steering Wheel Module - Stage 1 - Low Control
A2 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control | A2 | 0.5 TN | 3021 | Steering Wheel Module - Stage 1 - High Control
B1 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control | B1 | 0.5 PK | 3022 | Steering Wheel Module - Stage 2 - Low Control
B2 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control | B2 | 0.5 WH | 3023 | Steering Wheel Module - Stage 2 - High Control

### X302 Headliner Harness to Sun Roof Control Module

#### Connector Part Information

- OEM: 12092162
- Service: See Catalog
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12092163
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A-C: E/C
- Core/Insulation Crimp: Pins D: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X302 Headliner Harness to Sun Roof Control Module

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 750 | Ground | A | 0.5 WH | 750 | Ground
B | 0.5 L-BU | 131 | Sunroof Limit Switch | B | 0.5 YE | 131 | Sunroof Limit Switch
C | 0.5 L-GN | 129 | Sunroof Motor Close Control | C | 0.5 BK | 129 | Sunroof Motor Close Control
D | 0.5 D-GN/WH | 127 | Sunroof Motor Open Control | D | 0.5 D-GN | 127 | Sunroof Motor Open Control

### X305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness

#### Connector Part Information

- OEM: 12146437/12162144/12176335
- Service: 15305883/12102741/15305944
- Description: 4-Way F 150 (L-GY), 4-Way F 150 (BK), 8-Way F 280 Sealed (WH)

#### Connector Part Information

- OEM: 15326715
- Service: 15326715
- Description: 16-Way M Metri-Pack 150,150, 280 (GY) Series, Sealed

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A3, B3, C3, D3, F3, G3
- Terminal/Tray: 12034047/2
- Core/Insulation Crimp: Pins A3, C3: C/D
- Core/Insulation Crimp: Pins B3, D3, F3, G3: E/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

- Pins: A1, A2, B1, B2, C2, D2
- Terminal/Tray: 12047581/2
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 12094429/J-35616-3 (GY)

- Pins: H3
- Terminal/Tray: 12020116/2
- Core/Insulation Crimp: C/A
- Release Tool/Test Probe: 12094430/J-35616-5 (PU)

#### X305 EVAP Canister Purge Jumper Harness/Fuel Tank Harness/Wheel Speed Sensor Harness to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 RD/WH | 1840 | Battery Positive Voltage | 1A | 0.5 RD/WH | 1840 | Battery Positive Voltage
B | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control | 1B | 0.5 WH | 1310 | EVAP Canister Vent Solenoid Control
C-D | -- | -- | Not Used | 1C-1D | -- | -- | Not Used
A | 0.8 BN | 882 | Right Rear Wheel Speed Sensor Signal (JM4/JL4/JL9) | 2A | 0.5 BN | 882 | Right Rear Wheel Speed Sensor Signal (JM4/JL4/JL9)
B | 0.8 WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JM4/JL4/JL9) | 2B | 0.5 WH | 883 | Right Rear Wheel Speed Sensor Low Reference (JM4/JL4/JL9)
C | 0.8 BK | 884 | Left Rear Wheel Speed Sensor Signal (JM4/JL4/JL9) | 2C | 0.5 TN | 884 | Left Rear Wheel Speed Sensor Signal (JM4/JL4/JL9)
D | 0.8 RD | 885 | Left Rear Wheel Speed Sensor Low Reference (JM4/JL4/JL9) | 2D | 0.5 OG | 885 | Left Rear Wheel Speed Sensor Low Reference (JM4/JL4/JL9)
A | 0.35 BK | 850 | Ground | 3A | 1 BK | 850 | Ground
B | 0.5 TN | 510 | Fuel Sender Low Reference | 3B | 0.35 TN | 2759 | Fuel Sender Low Reference
C | 1 GY | 120 | Fuel Pump Supply Voltage | 3C | 1 GY | 120 | Fuel Pump Supply Voltage
D | 0.35 PU | 1589 | Fuel Level Sensor Signal | 3D | 0.35 PU | 1589 | Fuel Level Sensor Signal
E | -- | -- | Not Used | 3E | -- | -- | Not Used
F | 0.35 GY/BK | 2709 | 5-Volt Reference | 3F | 0.35 GY | 2709 | 5-Volt Reference
G | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal | 3G | 0.35 D-GN | 890 | Fuel Tank Pressure Sensor Signal
H | 0.5 BK/WH | 2759 | Fuel Tank Pressure Sensor Low Reference (L61/LE5) | 3H | 0.35 TN | 2759 | Fuel Tank Pressure Sensor Low Reference (L61/LE5)
3H | 0.35 TN | 2759 | Fuel Tank Pressure Sensor Low Reference (L61/LE5)

### X307 Body Harness to A/T Shift Control Module (MN5/MX0)

#### Connector Part Information

- OEM: 12047785
- Service: 12102900
- Description: 4-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047786
- Service: See Catalog
- Description: 4-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Pins: A-D
- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A-C: E/C
- Core/Insulation Crimp: Pins D: E/A
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X307 Body Harness to A/T Shift Control Module (MN5/MX0)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage | A | 0.35 WH | 8 | Instrument Panel Lamp Supply Voltage
B | 0.35 D-GN/WH | 1135 | A/T Shift Lock Control Solenoid Supply Voltage | B | 0.35 D-BU | 1135 | A/T Shift Lock Control Solenoid Supply Voltage
C | 0.5 D-GN/WH | 1932 | Transmission Shift Select Switch (Park) Signal | C | 0.5 YE | 1932 | Transmission Shift Select Switch (Park) Signal
D | 0.5 BK | 1250 | Ground | D | 0.5 BK | 1250 | Ground

### X314 Body Harness to the Passenger Seat Harness (KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326890
- Service: See Catalog
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X314 Body Harness to the Passenger Seat Harness (KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 1 RD/WH | 340 | Battery Positive Voltage | A | 1 RD/WH | 340 | Battery Positive Voltage
B | 0.35 L-BU/BK | 1505 | Passenger Heated Seat Switch Signal | B | 0.5 L-BU | 1505 | Passenger Heated Seat Switch Signal
C | 0.35 PK/BK | 1503 | Passenger Heated Seat High/Low Signal | C | 0.5 PK | 1503 | Passenger Heated Seat High/Low Signal
D | 0.8 BK | 1250 | Ground | D | 0.8 BK | 1250 | Ground

### X315 Body Harness to the Driver Seat Harness (KA1)

#### Connector Part Information

- OEM: 15326886
- Service: 88988300
- Description: 4-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326890
- Service: 88953361
- Description: 4-Way M GT 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins A, D: 2/A
- Core/Insulation Crimp: Pins B, C: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X315 Body Harness to the Driver Seat Harness (KA1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 1 RD/WH | 340 | Battery Positive Voltage | A | 1 RD/WH | 340 | Battery Positive Voltage
B | 0.35 L-BU | 1462 | Heated Seat Switch Signal | B | 0.5 L-BU | 1462 | Heated Seat Switch Signal
C | 0.35 PK | 1501 | Driver Heated Seat High/Low Signal | C | 0.5 PK | 1501 | Driver Heated Seat High/Low Signal
D | 0.8 BK | 1250 | Ground | D | 0.8 BK | 1250 | Ground

### X316 Body Harness to the Passenger Seat Harness

#### Connector Part Information

- OEM: 15332153
- Service: See Catalog
- Description: 10-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15332158
- Service: 88953270
- Description: 10-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Pins: A-G, J, K
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: H
- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X316 Body Harness to the Passenger Seat Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal | A | 0.35 OG | 1362 | Seat Belt Switch - Right - Signal
B | 0.35 PK | 915 | 5-Volt Reference | B | 0.35 PK/BK | 915 | 5-Volt Reference
C | 0.35 PK | 5057 | Low Reference | C | 0.35 BN | 5057 | Low Reference
D | 0.35 PK | 353 | Passenger Air Bag Off Indicator Control | D | 0.35 L-GN | 353 | Passenger Air Bag Off Indicator Control
E | 0.35 TN/BK | 723 | Passenger Air Bag On Indicator Control | E | 0.35 TN/BK | 723 | Passenger Air Bag On Indicator Control
F | 0.35 YE | 914 | Low Reference | F | 0.35 YE | 914 | Low Reference
G | 0.35 PK | 1339 | Ignition 1 Voltage | G | 0.35 PK | 1339 | Ignition 1 Voltage
H | 0.5 BK/WH | 1250 | Ground | H | 0.35 BK/WH | 1251 | Ground
J | 0.35 PK | 5018 | Occupant Sensor - Serial Data | J | 0.35 PU | 5018 | Occupant Sensor - Serial Data
K | 0.35 D-BU | 913 | Passenger Seat Belt Tension Sensor Signal | K | 0.35 D-BU | 913 | Passenger Seat Belt Tension Sensor Signal

### X319 Body Harness to Left Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12110505
- Service: 15306044
- Description: 2-Way F Metri-Pack 150 Series (YE)

#### Connector Part Information

- OEM: 12160816
- Service: 15306370
- Description: 2-Way M Metri-Pack 150 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X319 Body Harness to Left Roof Rail Module Harness (ASF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 PU/WH | 5019 | Roof Rail Module - Left - High Control | A | 0.5 D-GN | 5019 | Roof Rail Module - Left - High Control
B | 0.5 PK | 5020 | Roof Rail Module - Left - Low Control | B | 0.5 WH | 5020 | Roof Rail Module - Left - Low Control

### X320 Body Harness to Right Roof Rail Module Harness (ASF)

#### Connector Part Information

- OEM: 12110505
- Service: 15306044
- Description: 2-Way F Metri-Pack 150 Series (YE)

#### Connector Part Information

- OEM: 12160816
- Service: 15306370
- Description: 2-Way M Metri-Pack 150 Series (YE)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X320 Body Harness to Right Roof Rail Module Harness (ASF)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 YE/BK | 5021 | Roof Rail Module - Right - High Control | A | 0.5 D-GN | 5021 | Roof Rail Module - Right - High Control
B | 0.5 WH/BK | 5022 | Roof Rail Module - Right - Low Control | B | 0.5 WH | 5022 | Roof Rail Module - Right - Low Control

### X321 Body Harness to the Headliner Harness (UE1)

#### Connector Part Information

- OEM: 15336219
- Service: 15336219
- Description: 16-Way F GT 150, 280 Series

#### Connector Part Information

- OEM: 15336224
- Service: 15336224
- Description: 16-Way M GT 150, 280 Series

#### Terminal Part Information

- Pins: C, F, G, K, M, N, P, R
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: Pins C: C/A
- Core/Insulation Crimp: Pins F, G, K, M, N, P, R: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, H, J
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins J: 2/A
- Core/Insulation Crimp: Pins A, H: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: S
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: C, F, G, K, M, N, P, R
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins C: 2/4
- Core/Insulation Crimp: Pins R: E/4
- Core/Insulation Crimp: Pins F, G, K, M, N, P: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A, H
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: J, S
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins J: 2/A
- Core/Insulation Crimp: Pins S: A/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X321 Body Harness to the Headliner Harness (UE1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 GY | 157 | Courtesy Lamp Control | A | 0.5 GY | 157 | Courtesy Lamp Control
B | -- | -- | Not Used | B | -- | -- | Not Used
C | 0.8 BK | 750 | Ground | C | 0.5 BK | 750 | Ground
D-E | -- | -- | Not Used | D-E | -- | -- | Not Used
F | 0.35 D-GN/WH | 2514 | Keypad Signal | F | 0.35 D-GN/WH | 2514 | Keypad Signal
G | 0.35 L-GN/BK | 2515 | Keypad Supply Voltage | G | 0.35 L-GN/BK | 2515 | Keypad Supply Voltage
H | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage | H | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
J | 1 D-GN | 1301 | RAP Fuse Supply Voltage | J | 1 D-GN | 1301 | RAP Fuse Supply Voltage (CF5)
K | 0.35 BN/WH | 2517 | Keypad Red LED | K | 0.35 BN/WH | 2517 | Keypad Red LED
L | -- | -- | Not Used | L | -- | -- | Not Used
M | 0.35 YE/BK | 2516 | Keypad Green LED | M | 0.35 YE/BK | 2516 | Keypad Green LED
N | 0.35 GY | 655 | Cellular Telephone Microphone Signal | N | 0.35 GY | 655 | Cellular Telephone Microphone Signal
P | BARE | 1489 | Drain Wire | P | BARE | 1489 | Drain Wire
R-S | -- | -- | Not Used | R-S | -- | -- | Not Used

### X321 Body Harness to the Headliner Harness (without UE1)

#### Connector Part Information

- OEM: 15326900
- Service: 15306380
- Description: 6-Way F GT 280 Series (BK)

#### Connector Part Information

- OEM: 15326904
- Service: 88988314
- Description: 6-Way M GT 280 Series (BK)

#### Terminal Part Information

- Pins: C, B, D, E
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: Pins C, E: 2/A
- Core/Insulation Crimp: Pins B, D: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: B, C, D
- Terminal/Tray: 15304722/8
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

- Pins: A, E
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins E: 2/A
- Core/Insulation Crimp: Pins A: A/D
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X321 Body Harness to the Headliner Harness (without UE1)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | 0.5 GY | 157 | Interior Lamp Control | B | 0.5 GY | 157 | Interior Lamp Control
C | 0.8 BK | 750 | Ground | C | 0.35 BK | 750 | Ground
D | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage | D | 0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
0.5 D-BU/WH | 149 | Courtesy Lamp Supply Voltage
E | 1 D-GN | 1301 | Retained Accessory Power Fuse Supply Voltage | E | 1 D-GN | 1301 | Retained Accessory Power Fuse Supply Voltage (CF5)
F | -- | -- | Not Used | F | -- | -- | Not Used

### X400 Battery Cable to the Body Harness

#### Connector Part Information

- OEM: 12160893
- Service: 15306159
- Description: 1-Way F Metri-Pack 800 Series (BK)

#### Connector Part Information

- OEM: 12160894
- Service: See Catalog
- Description: 1-Way M Metri-Pack 800 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12092445/18
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: 12150860/J-35616-44 (YE)

#### Terminal Part Information

- Terminal/Tray: 12110700/24
- Core/Insulation Crimp: G/3/5
- Release Tool/Test Probe: 12150860/J-35616-45 (YE)

#### X400 Battery Cable to the Body Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 5 RD | 1 | Battery Positive Voltage | A | 5 RD | 1 | Battery Positive Voltage

### X401 Body Harness to the Rear Compartment Lamp Harness

#### Connector Part Information

- OEM: 12047662
- Service: 12085535
- Description: 2-Way F Metri-Pack 150 Series (BK)

#### Connector Part Information

- OEM: 12047663
- Service: 12085481
- Description: 2-Way M Metri-Pack 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12047767/2
- Core/Insulation Crimp: Pins A: E/A
- Core/Insulation Crimp: Pins B: E/C
- Release Tool/Test Probe: 12094429/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X401 Body Harness to the Rear Compartment Lamp Harness

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BK | 750 | Ground | A | 0.35 BK | 750 | Ground
B | 0.35 OG/BK | 737 | Rear Compartment Lamp Control | B | 0.35 OG/BK | 737 | Rear Compartment Lamp Control

### X492 Body Harness to the Left Rear Tail Lamp Assembly Harness (Sedan)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: Pins A: 2/A
- Core/Insulation Crimp: Pins B, C, D: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X492 Body Harness to the Left Rear Tail Lamp Assembly Harness (Sedan)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 750 | Ground | A | 0.5 BK | 750 | Ground
B | 0.5 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage | B | 0.5 YE | 18 | Left Rear Stop/Turn Lamp Supply Voltage
C | 0.5 BN | 9 | Park Lamp Supply Voltage | C | 0.5 BN | 9 | Park Lamp Supply Voltage
D | 0.5 L-GN | 24 | Backup Lamp Supply Voltage | D | 0.35 L-GN | 24 | Backup Lamp Supply Voltage

### X493 Body Harness to the Right Rear Tail Lamp Assembly Harness (Sedan)

#### Connector Part Information

- OEM: 15326815
- Service: 15306396
- Description: 4-Way F GT 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15326820
- Service: 15326820
- Description: 4-Way M GT 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: 12191819/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X493 Body Harness to the Right Rear Tail Lamp Assembly Harness (Sedan)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 BK | 850 | Ground | A | 0.5 BK | 850 | Ground
B | 0.5 D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage | B | 0.5 D-GN | 19 | Right Rear Stop/Turn Lamp Supply Voltage
C | 0.5 BN | 9 | Park Lamp Supply Voltage | C | 0.5 BN | 9 | Park Lamp Supply Voltage
D | 0.5 L-GN | 24 | Backup Lamp Supply Voltage | D | 0.35 L-GN | 24 | Backup Lamp Supply Voltage

### X494 License and Backup Lamp Harness to the Body Harness (G5)

#### Connector Part Information

- OEM:12160482
- Service: 12160482
- Description: 4-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 15499806
- Service: 15499806
- Description: 4-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X494 License and Backup Lamp Harness to the Body Harness (G5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Supply Voltage | A | 0.5 L-GN | 24 | Backup Lamp Supply Voltage
B | 0.5 BN | 9 | Park Lamp Supply Voltage | B | 0.5 BN | 9 | Park Lamp Supply Voltage
C | 0.8 BK | 750 | Ground | C | 0.8 BK | 750 | Ground
D | -- | -- | Not Used | D | -- | -- | Not Used

### X495 License Lamp Harness to Right Backup Lamp Assembly (G5)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052647
- Service: 12125649
- Description: 2-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X495 License Lamp Harness to Right Backup Lamp Assembly (G5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Supply Voltage | A | 0.5 BK | 24 | Backup Lamp Supply Voltage
B | 0.35 BK | 750 | Ground | B | 0.35 BK | 750 | Ground

### X496 License Lamp Harness to Left Backup Lamp Assembly (G5)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052647
- Service: 12125649
- Description: 2-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X496 License Lamp Harness to Left Backup Lamp Assembly (G5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.5 L-GN | 24 | Backup Lamp Supply Voltage | A | 0.5 BK | 24 | Backup Lamp Supply Voltage
B | 0.35 BK | 750 | Ground | B | 0.35 BK | 750 | Ground

### X497 License Lamp Harness to License Lamp Assembly (G5)

#### Connector Part Information

- OEM: 12052641
- Service: 12102747
- Description: 2-Way F Metri-Pack 150 Series Sealed (BK)

#### Connector Part Information

- OEM: 12052647
- Service: 12125649
- Description: 2-Way M Metri-Pack 150 Series Sealed (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X497 License Lamp Harness to License Lamp Assembly (G5)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 0.35 BN | 9 | Tail/License Lamps Supply Voltage | A | 0.35 BN | 9 | Tail/License Lamps Supply Voltage
B | 0.35 BK | 750 | Ground | B | 0.35 BK | 750 | Ground

### X500 Body Harness to the Driver Door Harness (AU3/DG7)

#### Connector Part Information

- OEM: 15401211
- Service: 88953323
- Description: 40-Way F GT 150, 280 Series (GY)

#### Connector Part Information

- OEM: 15401208
- Service: 88956505
- Description: 40-Way M GT 150, 280 Series (GY)

#### Terminal Part Information

- Pins: A1, B3, B5, B6, B11, B12, C3, C6-C8
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A2, A4, A5
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: A3, A6, A7, D2-D7
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: Pins A6: 4/4
- Core/Insulation Crimp: Pins: A3, A7, D2-D7: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: A1, B3, B5, B6, B11, B12, C3, C6-C8
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins B3, B5, B6: E/4
- Core/Insulation Crimp: Pins A1, B11, B12, C3, C6-C8: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A2-A7, D2-D7
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins A3, A7, D2-D7: A/D
- Core/Insulation Crimp: Pins A6: C/D
- Core/Insulation Crimp: Pins A2, A4, A5: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X500 Body Harness to the Driver Door Harness (AU3/DG7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | 0.35 GY/BK | 8 | Instrument Panel Lamp Supply Voltage | A1 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
A2 | 0.35 GY/BK | 8 | Instrument Panel Lamp Supply Voltage | A2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
A3 | 2 D-BU | 1307 | Power Window Master Switch Lockout Signal (Sedan) | A3 | 2 D-BU | 1307 | Power Window Master Switch Lockout Signal (Sedan)
A4 | 0.5 GY/BK | 118 | Left Front Speaker Output (-) (UQ3) | A4 | 0.5 GY/BK | 118 | Left Front Speaker Output (-) (UQ3)
A4 | 0.5 GY | 118 | Left Front Speaker Output (-) (UQ3)
A4 | 0.35 GY | 118 | Left Front Speaker Output (-) (UQ4) | A4 | 0.5 GY | 118 | Left Front Speaker Output (-) (UQ4)
A5 | 0.5 TN/BK | 201 | Left Front Speaker Output (+) (UQ3) | A5 | 0.5 TN | 201 | Left Front Speaker Output (+) (UQ3)
A5 | 0.5 TN | 201 | Left Front Speaker Output (+) (UQ3)
A5 | 0.35 TN | 201 | Left Front Speaker Output (+) (UQ4) | A5 | 0.5 TN | 201 | Left Front Speaker Output (+) (UQ4)
A6 | 2 BK | 1250 | Ground | A6 | 2 BK | 1250 | Ground
A7 | 3 D-GN | 801 | RAP Fuse Supply Voltage | A7 | 3 D-GN | 801 | RAP Fuse Supply Voltage
A8 | -- | -- | Not Used | A8 | -- | -- | Not Used
B1-B2 | -- | -- | Not Used | B1-B2 | -- | -- | Not Used
B3 | 0.35 WH | 682 | Door Lock Lock/Unlock Signal | B3 | 0.5 WH | 682 | Door Lock Lock/Unlock Signal
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control | B5 | 0.5 TN | 694 | Driver Door Lock Actuator Unlock Control
B6 | 0.5 GY | 295 | Door Lock Actuator Lock Control | B6 | 0.5 GY | 295 | Door Lock Actuator Lock Control
B7-B10 | -- | -- | Not Used | B7-B10 | -- | -- | Not Used
B11 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF) | B11 | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF)
B12 | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF) | B12 | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF)
C1-C2 | -- | -- | Not Used | C1-C2 | -- | -- | Not Used
C3 | 0.35 RD/WH | 440 | Battery Positive Voltage | C3 | 0.35 RD/WH | 440 | Battery Positive Voltage
C4-C5 | -- | -- | Not Used | C4-C5 | -- | -- | Not Used
C6 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control | C6 | 0.35 PU/WH | 889 | Passenger Mirror Motor Down Control
C7 | 0.35 WH | 330 | Passenger Mirror Motor Supply Voltage | C7 | 0.35 WH | 330 | Passenger Mirror Motor Supply Voltage (Coupe)
0.35 WH/BK | 330 | Passenger Mirror Motor Supply Voltage (Sedan)
C8 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control | C8 | 0.35 OG/WH | 881 | Passenger Mirror Motor Right Control
C9-C12 | -- | -- | Not Used | C9-C12 | -- | -- | Not Used
D1 | -- | -- | Not Used | D1 | -- | -- | Not Used
D2 | 3 L-BU | 166 | Power Window Master Switch Right Front Up Signal | D2 | 3 L-BU | 166 | Power Window Master Switch Right Front Up Signal
D3 | 3 TN | 167 | Power Window Master Switch Right Front Down Signal | D3 | 3 TN | 167 | Power Window Master Switch Right Front Down Signal
D4 | 3 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (Sedan) | D4 | 2 D-GN/YE | 168 | Power Window Master Switch Left Rear Up Signal (Sedan)
D5 | 3 PU | 169 | Power Window Master Switch Left Rear Down Signal (Sedan) | D5 | 2 PU | 169 | Power Window Master Switch Left Rear Down Signal (Sedan)
D6 | 3 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (Sedan) | D6 | 2 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (Sedan)
D7 | 3 PU | 171 | Power Window Master Switch Right Rear Down Signal (Sedan) | D7 | 2 PU/WH | 171 | Power Window Master Switch Right Rear Down Signal (Sedan)
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### X500 Body Harness to the Left Front Door Harness (without AU3/DG7)

#### Connector Part Information

- OEM: 15336205
- Service: See Catalog
- Description: 12-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15336209
- Service: See Catalog
- Description: 12-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X500 Body Harness to the Left Front Door Harness (without AU3/DG7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF) | B | 0.35 WH | 2132 | Side Impact Sensing Module - Left - Signal (ASF)
C | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF) | C | 0.35 YE | 2131 | Side Impact Sensing Module - Left - Voltage (ASF)
D-J | -- | -- | Not Used | D-J | -- | -- | Not Used
K | 0.35 GY | 118 | Left Front Speaker Output (-) | K | 0.5 GY | 118 | Left Front Speaker Output (-)
L | 0.35 TN/BK | 201 | Left Front Speaker Output (+) | L | 0.5 TN/BK | 201 | Left Front Speaker Output (+)
M | -- | -- | Not Used | M | -- | -- | Not Used

### X600 Body Harness to the Passenger Door Harness (AU3/DG7)

#### Connector Part Information

- OEM: 15401211
- Service: 88953323
- Description: 40-Way F GT 150, 280 Series (GY)

#### Connector Part Information

- OEM: 15401208
- Service: 88956505
- Description: 40-Way M GT 150, 280 Series (GY)

#### Terminal Part Information

- Pins: B3, B5-B8, B11, B12, C7
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A2, D4-D6
- Terminal/Tray: 15304711/8
- Core/Insulation Crimp: E/A
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

- Pins: D2, D3, D7
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Pins: B3, B5-B8, B11, B12, C7
- Terminal/Tray: 15304702/19
- Core/Insulation Crimp: Pins B3, B5, B6: E/4
- Core/Insulation Crimp: Pins B7, B8, B11, B12, C7: E/C
- Release Tool/Test Probe: 15315247/J-35616-3 (GY)

- Pins: A2, D2-D7
- Terminal/Tray: 15304724/8
- Core/Insulation Crimp: Pins D2, D3, D7: A/D
- Core/Insulation Crimp: Pins A2, D4-D6: See Terminal Repair Kit
- Release Tool/Test Probe: 15315247/J-35616-5 (PU)

#### X600 Body Harness to the Passenger Door Harness (AU3/DG7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | -- | -- | Not Used | A1 | -- | -- | Not Used
A2 | 0.35 GY/BK | 8 | Instrument Panel Lamp Supply Voltage | A2 | 0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
0.35 GY | 8 | Instrument Panel Lamp Supply Voltage
A3-A8 | -- | -- | Not Used | A3-A8 | -- | -- | Not Used
B1-B2 | -- | -- | Not Used | B1-B2 | -- | -- | Not Used
B3 | 0.35 WH | 682 | Door Lock Lock/Unlock Signal | B3 | 0.5 WH | 682 | Door Lock Lock/Unlock Signal
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | 0.5 TN | 294 | Door Lock Actuator Unlock Control | B5 | 0.5 TN | 294 | Door Lock Actuator Unlock Control
B6 | 0.5 GY | 295 | Door Lock Actuator Lock Control | B6 | 0.5 GY | 295 | Door Lock Actuator Lock Control
B7 | 0.35 OG/WH | 881 | Right Mirror Motor Right Control | B7 | 0.35 OG/WH | 881 | Right Mirror Motor Right Control
B8 | 0.35 PU/WH | 889 | Right Mirror Motor Down Control | B8 | 0.35 PU/WH | 889 | Right Mirror Motor Down Control
B9-B10 | -- | -- | Not Used | B9-B10 | -- | -- | Not Used
B11 | 0.35 D-GN | 2134 | Right Front Side Impact Sensing Module Signal (ASF) | B11 | 0.35 D-GN | 2134 | Right Front Side Impact Sensing Module Signal (ASF)
B12 | 0.35 TN | 2133 | Right Front Side Impact Sensing Module Supply Voltage (ASF) | B12 | 0.35 TN | 2133 | Right Front Side Impact Sensing Module Supply Voltage (ASF)
C1-C6 | -- | -- | Not Used | C1-C6 | -- | -- | Not Used
C7 | 0.35 WH | 330 | Right Mirror Motor Supply Voltage | C7 | 0.35 WH | 330 | Right Mirror Motor Supply Voltage
C8-C12 | -- | -- | Not Used | C8-C12 | -- | -- | Not Used
D1 | -- | -- | Not Used | D1 | -- | -- | Not Used
D2 | 3 L-BU | 166 | Power Window Master Switch Right Front Up Signal | D2 | 2 L-BU | 166 | Power Window Master Switch Right Front Up Signal
D3 | 3 TN | 167 | Power Window Master Switch Right Front Down Signal | D3 | 2 TN | 167 | Power Window Master Switch Right Front Down Signal
D4 | 0.5 D-GN/BK | 117 | Right Front Speaker Output (-) (UQ3) | D4 | 0.5 D-GN | 117 | Right Front Speaker Output (-) (UQ3)
D4 | 0.5 D-GN | 117 | Right Front Speaker Output (-) (UQ3)
D4 | 0.35 D-GN | 117 | Right Front Speaker Output (-) (UQ4) | D4 | 0.5 D-GN | 117 | Right Front Speaker Output (-) (UQ4)
D5 | 0.5 L-GN/BK | 200 | Right Front Speaker Output (+) (UQ3) | D5 | 0.5 L-GN | 200 | Right Front Speaker Output (+) (UQ3)
D5 | 0.5 L-GN | 200 | Right Front Speaker Output (+) (UQ3)
D5 | 0.35 L-GN | 200 | Right Front Speaker Output (+) (UQ4) | D5 | 0.5 L-GN | 200 | Right Front Speaker Output (+) (UQ4)
D6 | 0.5 BK | 1250 | Ground | D6 | 0.5 BK | 1250 | Ground
0.5 BK | 1250 | Ground
D7 | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage | D7 | 3 D-GN | 801 | Retained Accessory Power Fuse Supply Voltage
D8 | -- | -- | Not Used | D8 | -- | -- | Not Used

### X600 Body Harness to the Right Front Door Harness (without AU3/DG7)

#### Connector Part Information

- OEM: 15336205
- Service: See Catalog
- Description: 12-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15336209
- Service: See Catalog
- Description: 12-Way M GT 150, 280 Series (BK)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X600 Body Harness to the Right Front Door Harness (without AU3/DG7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF) | B | 0.35 D-GN | 2134 | Side Impact Sensing Module - Right - Signal (ASF)
C | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF) | C | 0.35 TN | 2133 | Side Impact Sensing Module - Right - Voltage (ASF)
D-J | -- | -- | Not Used | D-J | -- | -- | Not Used
K | 0.35 D-GN | 117 | Right Front Speaker Output (-) | K | 0.5 D-GN | 117 | Right Front Speaker Output (-)
L | 0.35 L-GN | 200 | Right Front Speaker Output (+) | L | 0.5 L-GN | 200 | Right Front Speaker Output (+)
M | -- | -- | Not Used | M | -- | -- | Not Used

### X700 Body Harness to the Left Rear Door Harness (Sedan with AU3/DG7)

#### Connector Part Information

- OEM: 15336212
- Service: 22715954
- Description: 14-Way F GT 150, 280 Series

#### Connector Part Information

- OEM: 15479759
- Service: See Catalog
- Description: 14-Way M GT 150, 280 Series

#### Terminal Part Information

- Pins: B, C
- Terminal/Tray: 12191812/19
- Core/Insulation Crimp: E/C
- Release Tool/Test Probe: 15315247/J-35616-2A (GY)

- Pins: A, G, H
- Terminal/Tray: 15304713/19
- Core/Insulation Crimp: F/D
- Release Tool/Test Probe: 15315247/J-35616-4A (PU)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X700 Body Harness to the Left Rear Door Harness (Sedan with AU3/DG7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 D-BU | 1307 | Power Window Master Switch Lockout Signal | A | 2 D-BU/WH | 1307 | Power Window Master Switch Lockout Signal (A31)
B | 0.5 TN | 294 | Door Lock Actuator Unlock Control | B | 0.5 TN | 294 | Door Lock Actuator Unlock Control
C | 0.5 GY | 295 | Door Lock Actuator Lock Control | C | 0.5 GY | 295 | Door Lock Actuator Lock Control
D-F | -- | -- | Not Used | D-F | -- | -- | Not Used
G | 3 D-GN | 168 | Power Window Master Switch Left Rear Up Signal | G | 2 D-GN | 168 | Power Window Master Switch Left Rear Up Signal (A31)
H | 3 PU | 169 | Power Window Master Switch Left Rear Down Signal | H | 2 PU | 169 | Power Window Master Switch Left Rear Down Signal (A31)
J-P | -- | -- | Not Used | J-P | -- | -- | Not Used

### X800 Body Harness to the Right Rear Door Harness (Sedan with AU3/DG7)

#### Connector Part Information

- OEM: 15336211
- Service: 22715954
- Description: 14-Way F GT 150, 280 Series (BK)

#### Connector Part Information

- OEM: 15479759
- Service: See Catalog
- Description: 14-Way M GT 150, 280 Series (GY)

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### Terminal Part Information

- Terminal/Tray: See Terminal Repair Kit
- Core/Insulation Crimp: See Terminal Repair Kit
- Release Tool/Test Probe: See Terminal Repair Kit

#### X800 Body Harness to the Right Rear Door Harness (Sedan with AU3/DG7)

Pin | Wire | Circuit | Function | Pin | Wire | Circuit | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | 3 D-BU | 1307 | Power Window Master Switch Lockout Signal | A | 2 D-BU/WH | 1307 | Power Window Master Switch Lockout Signal (A31)
B | 0.5 TN | 294 | Door Lock Actuator Unlock Control | B | 0.5 TN | 294 | Door Lock Actuator Unlock Control
C | 0.5 GY | 295 | Door Lock Actuator Lock Control | C | 0.5 GY | 295 | Door Lock Actuator Lock Control
D-F | -- | -- | Not Used | D-F | -- | -- | Not Used
G | 3 L-GN | 170 | Power Window Master Switch Right Rear Up Signal | G | 2 L-GN | 170 | Power Window Master Switch Right Rear Up Signal (A31)
H | 3 PU | 171 | Power Window Master Switch Right Rear Down Signal | H | 2 PU | 171 | Power Window Master Switch Right Rear Down Signal (A31)
J-P | -- | -- | Not Used | J-P | -- | -- | Not Used