For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
A/C Compressor to Block Bolt | 20 N·m | 15 lb ft
Accessory Drive Belt Tensioner Bolt | 32 N·m | 24 lb ft
Balance Shaft Adjustable Chain Guide Bolt | 15 N·m | 11 lb ft
Balance Shaft Bearing Carrier to Block Bolt | 10 N·m | 89 lb in
Balance Shaft Fixed Chain Guide Bolt | 15 N·m | 11 lb ft
Balance Shaft Sprocket Bolt | 50 N·m | 37 lb ft
Baro Sensor and Coolant Return Line Assembly | 8 N·m | 71 lb in
Boost Solenoid Bracket Nut | 10 N·m | 89 lb in
Cam Cover to Cylinder Head Bolt | 8 N·m | 71 lb in
Cam Cover to Ground Cable Bolt | 10 N·m | 89 lb in
Cam Cover to Ground Cable Stud | 10 N·m | 89 lb in
Cam Sensor Bolt | 8 N·m | 71 lb in
Camshaft

- Camshaft Position Sensor Housing Stud

22 N·m

16 lb ft

- Camshaft Bearing Cap Bolt

10 N·m

89 lb in

- Camshaft Sprocket Bolt -- First Pass

85 N·m

63 lb ft

- Camshaft Sprocket Bolt -- Final Pass

30 degrees

- Camshaft Timing Chain Tensioner

75 N·m

55 lb ft

- Intake Camshaft Rear Cap Bolt

25 N·m

18 lb ft

Chain Guide Access Hole Plug | 90 N·m | 59 lb ft
Connecting Rod Bolts

- First Pass

25 N·m

18 lb ft

- Final Pass

100 degrees

Crankshaft Bearing Lower Crankcase to Block Bolts

- First Pass

20 N·m

15 lb ft

- Final Pass

70 degrees

Crankshaft Position Reluctor Ring | 15 N·m | 11 lb ft
Crankshaft Position Sensor Bolt | 8 N·m | 71 lb in
Crankshaft Position Sensor Housing Studs | 22 N·m | 16 lb ft
Crankshaft Pulley Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

75 degrees

Cylinder Head Bolt

- First Pass

30 N·m

22 lb ft

- Final Pass

155 degrees

Cylinder Head Front Chaincase Bolt | 35 N·m | 26 lb ft
Cylinder Head Oil Gallery Plug | 35 N·m | 26 lb ft
Dipstick Guide to Intake Manifold Bolt | 10 N·m | 89 lb in
Elek. ICM Cover Bolt | 8 N·m | 71 lb in
Engine Coolant Temperature Sensor | 22 N·m | 16 lb ft
Engine Lift Bracket Front Bolt | 25 N·m | 18 lb ft
Engine Lift Bracket Rear Bolt | 25 N·m | 18 lb ft
Engine Mount Intermediate Bracket Bolts | 100 N·m | 74 lb ft
Engine Mount to Intermediate Bracket Bolts | 50 N·m | 37 lb ft
Engine Mount to Mid-Rail Nuts | 100 N·m | 74 lb ft
Exhaust Manifold to Cylinder Head Nut - 2 passes | 12 N·m | 106 lb in
Exhaust Manifold to Cylinder Head Stud | 10 N·m | 89 lb in
Exhaust Manifold Pipe Flange Stud | 16 N·m | 12 lb ft
Exhaust Takedown Pipe Nuts | 30 N·m | 22 lb ft
Flywheel (SMT) Bolt

- First Pass

53 N·m

39 lb ft

- Final Pass

25 degrees

Frame Bolts

- First Pass

100 N·m

74 lb ft

- Second Pass

180 degrees

Front Cover to Block Bolt | 25 N·m | 18 lb ft
Front Lift Bracket Bolt | 25 N·m | 18 lb ft
Fuel Feed Line | 14 N·m | 124 lb in
Fuel Feed Line and Injector Harness Bracket | 10 N·m | 89 lb in
Fuel Line Bracket Bolt | 10 N·m | 89 lb in
Fuel Pipe Bracket Bolt | 10 N·m | 89 lb in
Fuel Rail Bracket Stud | 10 N·m | 89 lb in
Generator Bracket Bolt | 42 N·m | 31 lb ft
Generator Connector Nut | 20 N·m | 15 lb ft
Generator to Block Bolt | 20 N·m | 15 lb ft
Heat Shield to Exhaust Manifold Bolt | 23 N·m | 17 lb ft
Idler Pulley | 22 N·m | 16 lb ft
Ignition Coil Bolt | 8 N·m | 71 lb in
Intake Manifold to Cylinder Head Bolt | 22 N·m | 16 lb ft
Intake Manifold to Cylinder Head Nut | 22 N·m | 16 lb ft
Intake Manifold to Cylinder Head Stud | 6 N·m | 53 lb in
Knock Sensor Bolt | 25 N·m | 18 lb ft
Lower Crankcase to Block Peripheral Bolts | 25 N·m | 18 lb ft
Oil Bypass Tube | 22 N·m | 16 lb ft
Oil Filter Housing Cover | 25 N·m | 18 lb ft
Oil Gallery Plug | 35 N·m | 26 lb ft
Oil Gallery Plug - Rear | 60 N·m | 44 lb ft
Oil Level Indicator Tube Bolt | 10 N·m | 89 lb in
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan to Block Bolts | 25 N·m | 18 lb ft
Oil Pressure Sensor | 18 N·m | 13 lb ft
Oil Pump Gerotor Cover Bolt | 6 N·m | 53 lb in
Oil Pump Pressure Relief Valve Plug | 40 N·m | 30 lb ft
Oxygen Sensor | 42 N·m | 31 lb ft
Power Steering Pump Blockout Plate Bolts | 25 N·m | 18 lb ft
Rear Lift Bracket Bolt | 22 N·m | 16 lb ft
Spark Plug | 20 N·m | 15 lb ft
Starter Motor to Block Bolt | 40 N·m | 30 lb ft
Starter Terminal Nut | 17 N·m | 13 lb ft
Supercharger Bolts | 25 N·m | 18 lb ft
Thermostat Housing to Block Bolts | 10 N·m | 89 lb in
Throttle Body Bolt | 10 N·m | 89 lb in
Timing Chain Adjustable Guide Bolt | 10 N·m | 89 lb in
Timing Chain Fixed Guide Bolt | 15 N·m | 11 lb ft
Timing Chain Oil Nozzle Bolt | 10 N·m | 89 lb in
Timing Chain Upper Guide Bolt | 10 N·m | 89 lb in
Torque Converter Bolts | 62 N·m | 46 lb ft
Transmission to Engine Bolts | 75 N·m | 55 lb ft
Vent Tube to Cylinder Head | 15 N·m | 11 lb ft
Water Pipe Support Bracket Bolt | 10 N·m | 89 lb in
Water Pump Access Cover Bolt | 7 N·m | 62 lb in
Water Pump/Balance Shaft Chain Tensioner Bolt | 10 N·m | 89 lb in
Water Pump Bolts | 25 N·m | 18 lb ft
Water Pump Drain Plug | 20 N·m | 15 lb ft
Water Pump Sprocket Bolt | 10 N·m | 89 lb in