For 1990-2009 cars

### Removal Procedure

1. Remove the console trim plate. Refer to Console Front Trim Plate Replacement .
2. If necessary, remove the shift control knob. Refer to Floor Shift Control Knob Replacement .
3. Remove the shift cable retaining clip.
4. Disconnect the shift cable from the shift control assembly.
5. Disconnect the shift lock solenoid harness connector (4).
6. Remove the shift control nuts (2).
7. Remove the shift control (3) from the vehicle.

### Installation Procedure

1. Install the shift control (3) to the vehicle.
2. Connect the shift lock solenoid harness connector (4).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the shift control nuts (2).

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

4. Connect the shift cable to the shift control assembly.
5. If the shift control knob was removed, install the shift control knob. Refer to Floor Shift Control Knob Replacement .
6. Install the console trim plate. Refer to Console Front Trim Plate Replacement .