For 1990-2009 cars

#### Tools Required

• | 87 90 800 Drift, Differential Seal

• | 87 91 311 Bearing Driver Shaft Sleeve

• | 87 92 236 Support

1. Remove the input shaft bearing retainer screws and the retainer.
2. Press out the input shaft bearing race using the 87 90 800 . Use the 87 92 236 as a base for the pressing operation.
3. Press out the output shaft bearing race using the 87 91 311 .
4. Remove the transaxle vent filter from the case using a punch. Drive the vent from the outside to the inside.