For 1990-2009 cars

### Removal Procedure

1. Remove the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .
2. Disconnect the washer fluid hose from the washer nozzle spouts.
3. Depress the washer nozzle tabs to disengage the nozzle from the air inlet grille.
4. Push the nozzles out from the air inlet grille panel opening.
5. Remove the windshield washer nozzles.

### Installation Procedure

1. Push the washer nozzles into the air inlet grille panel until the tabs engage with the panel.
2. Connect the washer fluid hose to both washer nozzle spouts.
3. Position the washer hose to the bottomside of the air inlet grille panel.
4. Install the air inlet grille panel. Refer to Air Inlet Grille Panel Replacement .