For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Remove the front seat. Refer to Front Seat Replacement - Bucket.
2. Remove the seat cushion frame. Refer to Front Seat Cushion Frame Replacement.
3. Re-zero the inflatable restraint passenger presence system whenever the seat cushion or any component of the passenger presence system is removed. Refer to Control Module References.

1 | Seat Cushion Cover

#### Procedure

1. Disconnect the seat cushion cover J-channel from the seat cushion frame.
2. Disconnect the electrical connectors.

2 | Seat Cushion Pad Tip The inflatable restraint passenger presence system is part of the seat cushion pad on the passenger seat, and must be replaced as an assembly.