For 1990-2009 cars

Callout | Component Name
--- | ---
Warning: Refer to SIR Inflator Module Handling and Storage Warning in the Preface section. Warning: Refer to SIR Warning in the Preface section.

#### Preliminary Procedures

1. Disable the supplemental inflatable restraint (SIR) system. Refer to SIR Disabling and Enabling.
2. On the sides of the steering wheel are 2 openings. Insert a small blunt-ended punch, or equivalent, through the access openings on the left and right of the steering wheel.
3. Push the spring fastener inward through the access hole. Repeat the step for the other opening.

1 | Steering Wheel Inflatable Restraint Module

#### Procedure

1. Remove the connector position assurance (CPA) retainer.
2. Disconnect the electrical connectors.
3. Fully deploy the module before disposal. If the module was replaced under warranty, fully deploy and dispose of the module after the required retention period. Refer to Inflator Module Handling and Scrapping.